## PanasonicRaw Tags

These tags are found in IFD0 of Panasonic/Leica RAW, RW2 and RWL images.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | PanasonicRawVersion | undef |
> 0x0002 | SensorWidth | no |
> 0x0003 | SensorHeight | no |
> 0x0004 | SensorTopBorder | no |
> 0x0005 | SensorLeftBorder | no |
> 0x0006 | SensorBottomBorder | no |
> 0x0007 | SensorRightBorder | no |
> 0x0008 | BlackLevel1 | int16u | (summing BlackLevel1+2+3 values gives the common bias that must be added to the BlackLevelRed/Green/Blue tags below)
> 0x0009 | BlackLevel2 | int16u |
> 0x000a | BlackLevel3 | int16u |
> 0x000e | LinearityLimitRed | int16u |
> 0x000f | LinearityLimitGreen | int16u |
> 0x0010 | LinearityLimitBlue | int16u |
> 0x0011 | RedBalance | int16u | (found in Digilux 2 RAW images)
> 0x0012 | BlueBalance | int16u |
> 0x0013 | WBInfo | - | --> PanasonicRaw WBInfo Tags
> 0x0017 | ISO | int16u |
> 0x0018 | HighISOMultiplierRed | int16u |
> 0x0019 | HighISOMultiplierGreen | int16u |
> 0x001a | HighISOMultiplierBlue | int16u |
> 0x001c | BlackLevelRed | int16u |
> 0x001d | BlackLevelGreen | int16u |
> 0x001e | BlackLevelBlue | int16u |
> 0x0024 | WBRedLevel | int16u |
> 0x0025 | WBGreenLevel | int16u |
> 0x0026 | WBBlueLevel | int16u |
> 0x0027 | WBInfo2 | - | --> PanasonicRaw WBInfo2 Tags
> 0x002e | JpgFromRaw | undef! | --> JPEG Tags (processed as an embedded document because it contains full EXIF)
> 0x002f | CropTop | int16u |
> 0x0030 | CropLeft | int16u |
> 0x0031 | CropBottom | int16u |
> 0x0032 | CropRight | int16u |
> 0x010f | Make | string |
> 0x0110 | Model | string |
> 0x0111 | StripOffsets | no |
> 0x0112 | Orientation | int16u |
> 1 = Horizontal (normal) 2 = Mirror horizontal 3 = Rotate 180 4 = Mirror vertical 5 = Mirror horizontal and rotate 270 CW 6 = Rotate 90 CW 7 = Mirror horizontal and rotate 90 CW 8 = Rotate 270 CW
> 0x0116 | RowsPerStrip | no |
> 0x0117 | StripByteCounts | no |
> 0x0118 | RawDataOffset | no |
> 0x0119 | DistortionInfo | - | --> PanasonicRaw DistortionInfo Tags
> 0x0120 | CameraIFD | - | --> PanasonicRaw CameraIFD Tags
> 0x02bc | ApplicationNotes | int8u! | --> XMP Tags
> 0x83bb | IPTC-NAA | int32u! | --> IPTC Tags
> 0x8769 | ExifOffset | - | --> EXIF Tags
> 0x8825 | GPSInfo | - | --> GPS Tags

## PanasonicRaw WBInfo Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | NumWBEntries | int16u |
> 1 | WBType1 | int16u | --> EXIF LightSource Values
> 2 | WB_RBLevels1 | int16u[2] |
> 4 | WBType2 | int16u | --> EXIF LightSource Values
> 5 | WB_RBLevels2 | int16u[2] |
> 7 | WBType3 | int16u | --> EXIF LightSource Values
> 8 | WB_RBLevels3 | int16u[2] |
> 10 | WBType4 | int16u | --> EXIF LightSource Values
> 11 | WB_RBLevels4 | int16u[2] |
> 13 | WBType5 | int16u | --> EXIF LightSource Values
> 14 | WB_RBLevels5 | int16u[2] |
> 16 | WBType6 | int16u | --> EXIF LightSource Values
> 17 | WB_RBLevels6 | int16u[2] |
> 19 | WBType7 | int16u | --> EXIF LightSource Values
> 20 | WB_RBLevels7 | int16u[2] |

## PanasonicRaw WBInfo2 Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | NumWBEntries | int16u |
> 1 | WBType1 | int16u | --> EXIF LightSource Values
> 2 | WB_RGBLevels1 | int16u[3] |
> 5 | WBType2 | int16u | --> EXIF LightSource Values
> 6 | WB_RGBLevels2 | int16u[3] |
> 9 | WBType3 | int16u | --> EXIF LightSource Values
> 10 | WB_RGBLevels3 | int16u[3] |
> 13 | WBType4 | int16u | --> EXIF LightSource Values
> 14 | WB_RGBLevels4 | int16u[3] |
> 17 | WBType5 | int16u | --> EXIF LightSource Values
> 18 | WB_RGBLevels5 | int16u[3] |
> 21 | WBType6 | int16u | --> EXIF LightSource Values
> 22 | WB_RGBLevels6 | int16u[3] |
> 25 | WBType7 | int16u | --> EXIF LightSource Values
> 26 | WB_RGBLevels7 | int16u[3] |

## PanasonicRaw DistortionInfo Tags

Lens distortion correction information.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0002 | DistortionParam02 | int16s |
> 0x0004 | DistortionParam04 | int16s |
> 0x0005 | DistortionScale | int16s |
> 7.1 | DistortionCorrection | int16s | [Mask 0x0f] 0x0 = Off 0x1 = On
> 0x0008 | DistortionParam08 | int16s |
> 0x0009 | DistortionParam09 | int16s |
> 0x000b | DistortionParam11 | int16s |
> 0x000c | DistortionN? | int16s |

## PanasonicRaw CameraIFD Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x1101 | FocusDistance | no |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Aug 9, 2017

<-- ExifTool Tag Names