## Nikon Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | MakerNoteVersion | undef[4] |
> 0x0002 | ISO | int16u[2] |
> 0x0003 | ColorMode | string |
> 0x0004 | Quality | string |
> 0x0005 | WhiteBalance | string |
> 0x0006 | Sharpness | string |
> 0x0007 | FocusMode | string |
> 0x0008 | FlashSetting | string |
> 0x0009 | FlashType | string |
> 0x000b | WhiteBalanceFineTune | int16s[n] |
> 0x000c | WB_RBLevels | rational64u[4] |
> 0x000d | ProgramShift | undef[4] |
> 0x000e | ExposureDifference | undef[4] |
> 0x000f | ISOSelection | string |
> 0x0010 | DataDump | no |
> 0x0011 | PreviewIFD | - | --> Nikon PreviewIFD Tags
> 0x0012 | FlashExposureComp | undef[4] | (may be set even if flash does not fire. Does not include the effect of flash bracketing.)
> 0x0013 | ISOSetting | int16u[2] |
> 0x0014 | ColorBalanceA NRWData? | - yes | --> Nikon ColorBalanceA Tags (large unknown block in NRW images, not copied to JPEG images)
> 0x0016 | ImageBoundary | int16u[4] |
> 0x0017 | ExternalFlashExposureComp | undef[4] |
> 0x0018 | FlashExposureBracketValue | undef[4] |
> 0x0019 | ExposureBracketValue | rational64s |
> 0x001a | ImageProcessing | string |
> 0x001b | CropHiSpeed | int16u[7]~ |
> 0x001c | ExposureTuning | undef[3] |
> 0x001d | SerialNumber | string! | (this value is used as a key to decrypt other information -- writing this tag causes the other information to be re-encrypted with the new key)
> 0x001e | ColorSpace | int16u | 1 = sRGB 2 = Adobe RGB
> 0x001f | VRInfo | - | --> Nikon VRInfo Tags
> 0x0020 | ImageAuthentication | int8u | 0 = Off 1 = On
> 0x0021 | FaceDetect | - | --> Nikon FaceDetect Tags
> 0x0022 | ActiveD-Lighting | int16u |
> 0 = Off 1 = Low 3 = Normal 5 = High 7 = Extra High |  | 8 = Extra High 1 9 = Extra High 2 10 = Extra High 3 11 = Extra High 4 65535 = Auto
> 0x0023 | PictureControlData | undef! | --> Nikon PictureControl Tags --> Nikon PictureControl2 Tags
> 0x0024 | WorldTime | - | --> Nikon WorldTime Tags
> 0x0025 | ISOInfo | - | --> Nikon ISOInfo Tags
> 0x002a | VignetteControl | int16u | 0 = Off 1 = Low 3 = Normal 5 = High
> 0x002b | DistortInfo | - | --> Nikon DistortInfo Tags
> 0x002c | UnknownInfo | - | --> Nikon UnknownInfo Tags
> 0x0032 | UnknownInfo2 | - | --> Nikon UnknownInfo2 Tags
> 0x0035 | HDRInfo | - | --> Nikon HDRInfo Tags
> 0x0039 | LocationInfo | - | --> Nikon LocationInfo Tags
> 0x003d | BlackLevel | int16u[4] |
> 0x004f | ColorTemperatureAuto | int16u |
> 0x0080 | ImageAdjustment | string |
> 0x0081 | ToneComp | string |
> 0x0082 | AuxiliaryLens | string |
> 0x0083 | LensType | int8u | Bit 0 = MF Bit 1 = D Bit 2 = G Bit 3 = VR
> 0x0084 | Lens | rational64u[4] |
> 0x0085 | ManualFocusDistance | rational64u |
> 0x0086 | DigitalZoom | rational64u |
> 0x0087 | FlashMode | int8u |
> 0 = Did Not Fire 1 = Fired, Manual 3 = Not Ready 7 = Fired, External 8 = Fired, Commander Mode 9 = Fired, TTL Mode
> 0x0088 | AFInfo | - | --> Nikon AFInfo Tags --> Nikon AFInfo Tags
> 0x0089 | ShootingMode | int16u~ | (for the D70, Bit 5 = Unused LE-NR Slowdown) Bit 0 = Continuous Bit 1 = Delay Bit 2 = PC Control Bit 3 = Self-timer Bit 4 = Exposure Bracketing Bit 5 = Auto ISO Bit 6 = White-Balance Bracketing Bit 7 = IR Control Bit 8 = D-Lighting Bracketing
> 0x008b | LensFStops | undef[4] |
> 0x008c | ContrastCurve | undef! |
> 0x008d | ColorHue | string |
> 0x008f | SceneMode | string |
> 0x0090 | LightSource | string |
> 0x0091 | ShotInfoD40 ShotInfoD80 ShotInfoD90 ShotInfoD3a ShotInfoD3b ShotInfoD3X ShotInfoD3S ShotInfoD300a ShotInfoD300b ShotInfoD300S ShotInfoD700 ShotInfoD800 ShotInfoD810 ShotInfoD850 ShotInfoD5000 ShotInfoD5100 ShotInfoD5200 ShotInfoD7000 ShotInfoD4 ShotInfoD4S ShotInfoD5 ShotInfoD500 ShotInfoD610 ShotInfo02xx ShotInfoUnknown | - - - - - - - - - - - - - - - - - - - - - - - - - | --> Nikon ShotInfoD40 Tags --> Nikon ShotInfoD80 Tags --> Nikon ShotInfoD90 Tags --> Nikon ShotInfoD3a Tags --> Nikon ShotInfoD3b Tags --> Nikon ShotInfoD3X Tags --> Nikon ShotInfoD3S Tags --> Nikon ShotInfoD300a Tags --> Nikon ShotInfoD300b Tags --> Nikon ShotInfoD300S Tags --> Nikon ShotInfoD700 Tags --> Nikon ShotInfoD800 Tags --> Nikon ShotInfoD810 Tags --> Nikon ShotInfoD850 Tags --> Nikon ShotInfoD5000 Tags --> Nikon ShotInfoD5100 Tags --> Nikon ShotInfoD5200 Tags --> Nikon ShotInfoD7000 Tags --> Nikon ShotInfoD4 Tags --> Nikon ShotInfoD4S Tags --> Nikon ShotInfoD500 Tags --> Nikon ShotInfoD500 Tags --> Nikon ShotInfoD610 Tags --> Nikon ShotInfo Tags --> Nikon ShotInfo Tags
> 0x0092 | HueAdjustment | int16s |
> 0x0093 | NEFCompression | int16u |
> 1 = Lossy (type 1) 2 = Uncompressed 3 = Lossless 4 = Lossy (type 2) 6 = Uncompressed (reduced to 12 bit) 8 = Small
> 0x0094 | Saturation | int16s |
> 0x0095 | NoiseReduction | string |
> 0x0096 | NEFLinearizationTable | undef! |
> 0x0097 | ColorBalance0100 ColorBalance0102 ColorBalance0103 ColorBalance0205 ColorBalance0209 ColorBalance02 ColorBalance0211 ColorBalance0213 ColorBalance0215 ColorBalanceUnknown02 ColorBalanceUnknown04 ColorBalanceUnknown | - - - - - - - - - - - - | --> Nikon ColorBalance1 Tags --> Nikon ColorBalance2 Tags --> Nikon ColorBalance3 Tags --> Nikon ColorBalance2 Tags --> Nikon ColorBalance4 Tags --> Nikon ColorBalance2 Tags --> Nikon ColorBalance4 Tags --> Nikon ColorBalance2 Tags --> Nikon ColorBalance4 Tags --> Nikon ColorBalanceUnknown Tags --> Nikon ColorBalanceUnknown Tags --> Nikon ColorBalanceUnknown Tags
> 0x0098 | LensData0100 LensData0101 LensData0201 LensData0204 LensData0400 LensDataUnknown | - - - - - - | --> Nikon LensData00 Tags --> Nikon LensData01 Tags --> Nikon LensData01 Tags --> Nikon LensData0204 Tags --> Nikon LensData0400 Tags --> Nikon LensDataUnknown Tags
> 0x0099 | RawImageCenter | int16u[2] |
> 0x009a | SensorPixelSize | rational64u[2] |
> 0x009c | SceneAssist | string |
> 0x009e | RetouchHistory | int16u[10] | [Values 0-9]
> 0 = None 3 = B & W 4 = Sepia 5 = Trim 6 = Small Picture 7 = D-Lighting 8 = Red Eye 9 = Cyanotype 10 = Sky Light 11 = Warm Tone 12 = Color Custom 13 = Image Overlay 14 = Red Intensifier 15 = Green Intensifier 16 = Blue Intensifier 17 = Cross Screen 18 = Quick Retouch 19 = NEF Processing 23 = Distortion Control 25 = Fisheye 26 = Straighten 29 = Perspective Control |  | 30 = Color Outline 31 = Soft Filter 32 = Resize 33 = Miniature Effect 34 = Skin Softening 35 = Selected Frame 37 = Color Sketch 38 = Selective Color 39 = Glamour 40 = Drawing 44 = Pop 45 = Toy Camera Effect 1 46 = Toy Camera Effect 2 47 = Cross Process (red) 48 = Cross Process (blue) 49 = Cross Process (green) 50 = Cross Process (yellow) 51 = Super Vivid 52 = High-contrast Monochrome 53 = High Key 54 = Low Key
> 0x00a0 | SerialNumber | string |
> 0x00a2 | ImageDataSize | int32u |
> 0x00a5 | ImageCount | int32u |
> 0x00a6 | DeletedImageCount | int32u |
> 0x00a7 | ShutterCount | int32u! | (this value is used as a key to decrypt other information -- writing this tag causes the other information to be re-encrypted with the new key)
> 0x00a8 | FlashInfo0100 FlashInfo0102 FlashInfo0103 FlashInfo0107 FlashInfoUnknown | - - - - - | --> Nikon FlashInfo0100 Tags --> Nikon FlashInfo0102 Tags --> Nikon FlashInfo0103 Tags --> Nikon FlashInfo0107 Tags --> Nikon FlashInfoUnknown Tags
> 0x00a9 | ImageOptimization | string |
> 0x00aa | Saturation | string |
> 0x00ab | VariProgram | string |
> 0x00ac | ImageStabilization | string |
> 0x00ad | AFResponse | string |
> 0x00b0 | MultiExposure | - | --> Nikon MultiExposure Tags --> Nikon MultiExposure Tags
> 0x00b1 | HighISONoiseReduction | int16u |
> 0 = Off 1 = Minimal 2 = Low 3 = Medium Low |  | 4 = Normal 5 = Medium High 6 = High
> 0x00b3 | ToningEffect | string |
> 0x00b6 | PowerUpTime | undef | (date/time when camera was last powered up)
> 0x00b7 | AFInfo2 | - | --> Nikon AFInfo2 Tags
> 0x00b8 | FileInfo | - | --> Nikon FileInfo Tags --> Nikon FileInfo Tags
> 0x00b9 | AFTune | - | --> Nikon AFTune Tags
> 0x00bb | RetouchInfo | - | --> Nikon RetouchInfo Tags
> 0x00bd | PictureControlData | undef! | --> Nikon PictureControl Tags
> 0x00c3 | BarometerInfo | - | --> Nikon BarometerInfo Tags
> 0x0e00 | PrintIM | - | --> PrintIM Tags
> 0x0e01 | NikonCaptureData | undef! | --> NikonCapture Tags (this data is dropped when copying Nikon MakerNotes since it may be too large to fit in the EXIF segment of a JPEG image, but it may be copied as a block into existing Nikon MakerNotes later if desired)
> 0x0e09 | NikonCaptureVersion | string |
> 0x0e0e | NikonCaptureOffsets | - | --> Nikon CaptureOffsets Tags
> 0x0e10 | NikonScanIFD | - | --> Nikon Scan Tags
> 0x0e13 | NikonCaptureEditVersions NikonCaptureEditVersions | undef undef! | (the ExtractEmbedded option may be used to decode settings from the stored edit versions, otherwise this is extracted as a binary data block) --> NikonCapture Tags
> 0x0e1d | NikonICCProfile | undef! | --> ICC_Profile Tags
> 0x0e1e | NikonCaptureOutput | undef! | --> Nikon CaptureOutput Tags
> 0x0e22 | NEFBitDepth | int16u[4]! | '0 0 0 0' = n/a (JPEG) '8 8 8 0' = 8 x 3 '12 0 0 0' = 12 '14 0 0 0' = 14 '16 16 16 0' = 16 x 3

## Nikon PreviewIFD Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x00fe | SubfileType | no | 0x0 = Full-resolution Image 0x1 = Reduced-resolution image 0x2 = Single page of multi-page image 0x3 = Single page of multi-page reduced-resolution image 0x4 = Transparency mask 0x5 = Transparency mask of reduced-resolution image 0x6 = Transparency mask of multi-page image 0x7 = Transparency mask of reduced-resolution multi-page image 0x10001 = Alternate reduced-resolution image 0xffffffff = invalid Bit 0 = Reduced resolution Bit 1 = Single page Bit 2 = Transparency mask Bit 3 = TIFF/IT final page Bit 4 = TIFF-FX mixed raster content
> 0x0103 | Compression | no | --> EXIF Compression Values
> 0x011a | XResolution | no |
> 0x011b | YResolution | no |
> 0x0128 | ResolutionUnit | no | 1 = None 2 = inches 3 = cm
> 0x0201 | PreviewImageStart | int32u* |
> 0x0202 | PreviewImageLength | int32u* |
> 0x0213 | YCbCrPositioning | no | 1 = Centered 2 = Co-sited

## Nikon ColorBalanceA Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 624 | RedBalance | int16u! |
> 625 | BlueBalance | int16u! |

## Nikon VRInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | VRInfoVersion | no |
> 4 | VibrationReduction | int8u | 0 = n/a 1 = On 2 = Off
> 6 | VRMode | int8u | 0 = Normal 2 = Active

## Nikon FaceDetect Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | FaceDetectFrameSize | int16u[2] |
> 3 | FacesDetected | int16u |
> 4 | Face1Position | int16u[4] | (top, left, width and height of face detect area in coordinates of FaceDetectFrameSize)
> 8 | Face2Position | int16u[4] |
> 12 | Face3Position | int16u[4] |
> 16 | Face4Position | int16u[4] |
> 20 | Face5Position | int16u[4] |
> 24 | Face6Position | int16u[4] |
> 28 | Face7Position | int16u[4] |
> 32 | Face8Position | int16u[4] |
> 36 | Face9Position | int16u[4] |
> 40 | Face10Position | int16u[4] |
> 44 | Face11Position | int16u[4] |
> 48 | Face12Position | int16u[4] |

## Nikon PictureControl Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | PictureControlVersion | no |
> 4 | PictureControlName | string[20] |
> 24 | PictureControlBase | string[20] |
> 48 | PictureControlAdjust | int8u | 0 = Default Settings 1 = Quick Adjust 2 = Full Control
> 49 | PictureControlQuickAdjust | int8u |
> 50 | Sharpness | int8u |
> 51 | Contrast | int8u |
> 52 | Brightness | int8u |
> 53 | Saturation | int8u |
> 54 | HueAdjustment | int8u |
> 55 | FilterEffect | int8u |
> 0x80 = Off 0x81 = Yellow 0x82 = Orange |  | 0x83 = Red 0x84 = Green 0xff = n/a
> 56 | ToningEffect | int8u |
> 0x80 = B&W 0x81 = Sepia 0x82 = Cyanotype 0x83 = Red 0x84 = Yellow 0x85 = Green |  | 0x86 = Blue-green 0x87 = Blue 0x88 = Purple-blue 0x89 = Red-purple 0xff = n/a
> 57 | ToningSaturation | int8u |

## Nikon PictureControl2 Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | PictureControlVersion | no |
> 4 | PictureControlName | string[20] |
> 24 | PictureControlBase | string[20] |
> 48 | PictureControlAdjust | int8u | 0 = Default Settings 1 = Quick Adjust 2 = Full Control
> 49 | PictureControlQuickAdjust | int8u |
> 51 | Sharpness | int8u |
> 53 | Clarity | int8u |
> 55 | Contrast | int8u |
> 57 | Brightness | int8u |
> 59 | Saturation | int8u |
> 61 | Hue | int8u |
> 63 | FilterEffect | int8u |
> 0x80 = Off 0x81 = Yellow 0x82 = Orange |  | 0x83 = Red 0x84 = Green 0xff = n/a
> 64 | ToningEffect | int8u |
> 0x80 = B&W 0x81 = Sepia 0x82 = Cyanotype 0x83 = Red 0x84 = Yellow 0x85 = Green |  | 0x86 = Blue-green 0x87 = Blue 0x88 = Purple-blue 0x89 = Red-purple 0xff = n/a
> 65 | ToningSaturation | int8u |

## Nikon WorldTime Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | TimeZone | int16s |
> 2 | DaylightSavings | int8u | 0 = No 1 = Yes
> 3 | DateDisplayFormat | int8u | 0 = Y/M/D 1 = M/D/Y 2 = D/M/Y

## Nikon ISOInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ISO | int8u | (val = 100 * 2**(raw/12-5))
> 4 | ISOExpansion | int16u |
> 0x0 = Off 0x101 = Hi 0.3 0x102 = Hi 0.5 0x103 = Hi 0.7 0x104 = Hi 1.0 0x105 = Hi 1.3 0x106 = Hi 1.5 0x107 = Hi 1.7 0x108 = Hi 2.0 0x109 = Hi 2.3 0x10a = Hi 2.5 0x10b = Hi 2.7 0x10c = Hi 3.0 |  | 0x10d = Hi 3.3 0x10e = Hi 3.5 0x10f = Hi 3.7 0x110 = Hi 4.0 0x111 = Hi 4.3 0x112 = Hi 4.5 0x113 = Hi 4.7 0x114 = Hi 5.0 0x201 = Lo 0.3 0x202 = Lo 0.5 0x203 = Lo 0.7 0x204 = Lo 1.0
> 6 | ISO2 | int8u | (val = 100 * 2**(raw/12-5))
> 10 | ISOExpansion2 | int16u |
> 0x0 = Off 0x101 = Hi 0.3 0x102 = Hi 0.5 0x103 = Hi 0.7 0x104 = Hi 1.0 0x105 = Hi 1.3 0x106 = Hi 1.5 |  | 0x107 = Hi 1.7 0x108 = Hi 2.0 0x201 = Lo 0.3 0x202 = Lo 0.5 0x203 = Lo 0.7 0x204 = Lo 1.0

## Nikon DistortInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | DistortionVersion? | no |
> 4 | AutoDistortionControl | int8u | 0 = Off 1 = On 2 = On (underwater)

## Nikon UnknownInfo Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | UnknownInfoVersion? | no |

## Nikon UnknownInfo2 Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | UnknownInfo2Version? | no |

## Nikon HDRInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | HDRInfoVersion | string[4] |
> 4 | HDR | int8u | 0 = Off 1 = On 48 = Auto
> 5 | HDRLevel | int8u | 0 = Auto 1 = 1 EV 2 = 2 EV 3 = 3 EV 255 = n/a
> 6 | HDRSmoothing | int8u |
> 0 = Off 1 = Normal 2 = Low |  | 3 = High 48 = Auto 255 = n/a
> 7 | HDRLevel2 | int8u | 0 = Auto 1 = 1 EV 2 = 2 EV 3 = 3 EV 255 = n/a

## Nikon LocationInfo Tags

Tags written by some Nikon GPS-equipped cameras like the AW100.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LocationInfoVersion | undef[4] |
> 4 | TextEncoding | int8u | 0 = n/a 1 = UTF8 2 = UTF16
> 5 | CountryCode | undef[3] |
> 8 | POILevel | int8u |
> 9 | Location | undef[70] |

## Nikon AFInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | AFAreaMode | int8u |
> 0 = Single Area 1 = Dynamic Area 2 = Dynamic Area (closest subject) 3 = Group Dynamic 4 = Single Area (wide) 5 = Dynamic Area (wide)
> 1 | AFPoint | int8u | (in some focus modes this value is not meaningful)
> 0 = Center 1 = Top 2 = Bottom 3 = Mid-left 4 = Mid-right 5 = Upper-left |  | 6 = Upper-right 7 = Lower-left 8 = Lower-right 9 = Far Left 10 = Far Right
> 2 | AFPointsInFocus | int16u |
> 0x0 = (none) 0x7ff = All 11 Points Bit 0 = Center Bit 1 = Top Bit 2 = Bottom Bit 3 = Mid-left Bit 4 = Mid-right |  | Bit 5 = Upper-left Bit 6 = Upper-right Bit 7 = Lower-left Bit 8 = Lower-right Bit 9 = Far Left Bit 10 = Far Right

## Nikon ShotInfoD40 Tags

These tags are extracted from encrypted data in D40 and D40X images.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 582 | ShutterCount | int32u |
> 586.1 | VibrationReduction | int8u | [Mask 0x08] 0x0 = Off 0x8 = On
> 729 | CustomSettingsD40 | - | --> NikonCustom SettingsD40 Tags

## Nikon ShotInfoD80 Tags

These tags are extracted from encrypted data in D80 images.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 586 | ShutterCount | int32u |
> 590.1 | Rotation | int8u | [Mask 0x07] 0x0 = Horizontal 0x1 = Rotate 270 CW 0x2 = Rotate 90 CW 0x3 = Rotate 180
> 590.2 | VibrationReduction | int8u | [Mask 0x18] 0x0 = Off 0x18 = On
> 590.3 | FlashFired | int8u | [Mask 0xe0] Bit 6 = Internal Bit 7 = External
> 708 | NikonImageSize | int8u | [Mask 0xf0] 0x0 = Large (10.0 M) 0x10 = Medium (5.6 M) 0x20 = Small (2.5 M)
> 708.1 | ImageQuality | int8u | [Mask 0x0f]
> 0x0 = NEF (RAW) 0x1 = JPEG Fine 0x2 = JPEG Normal 0x3 = JPEG Basic 0x4 = NEF (RAW) + JPEG Fine 0x5 = NEF (RAW) + JPEG Normal 0x6 = NEF (RAW) + JPEG Basic
> 748 | CustomSettingsD80 | - | --> NikonCustom SettingsD80 Tags

## Nikon ShotInfoD90 Tags

These tags are extracted from encrypted data in images from the D90 with firmware 1.00.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 693 | ISO2 | int8u |
> 725 | ShutterCount | int32u |
> 884 | CustomSettingsD90 | - | --> NikonCustom SettingsD90 Tags

## Nikon ShotInfoD3a Tags

These tags are extracted from encrypted data in images from the D3 with firmware 1.00 and earlier.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 598 | ISO2 | int8u |
> 630 | ShutterCount | int32u |
> 723.1 | NikonImageSize | int8u | [Mask 0x18] 0x0 = Large 0x8 = Medium 0x10 = Small
> 723.2 | ImageQuality | int8u | [Mask 0x07]
> 0x0 = NEF (RAW) + JPEG Fine 0x1 = NEF (RAW) + JPEG Norm 0x2 = NEF (RAW) + JPEG Basic 0x3 = NEF (RAW) 0x4 = TIF (RGB) 0x5 = JPEG Fine 0x6 = JPEG Normal 0x7 = JPEG Basic
> 769 | CustomSettingsD3 | - | --> NikonCustom SettingsD3 Tags

## Nikon ShotInfoD3b Tags

These tags are extracted from encrypted data in images from the D3 with firmware 1.10, 2.00, 2.01 and 2.02.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 16 | ImageArea | int8u | 0 = FX (36.0 x 23.9 mm) 1 = DX (23.5 x 15.6 mm) 2 = 5:4 (30.0 x 23.9 mm)
> 605 | ISO2 | int8u |
> 637 | ShutterCount | int32u | (firmware 1.10)
> 639 | ShutterCount | int32u | (firmware 2.00, 2.01 and 2.02)
> 650 | PreFlashReturnStrength | int8u | (valid in TTL and TTL-BL flash control modes)
> 732.1 | NikonImageSize | int8u | [Mask 0x18] 0x0 = Large 0x8 = Medium 0x10 = Small
> 732.2 | ImageQuality | int8u | [Mask 0x07]
> 0x0 = NEF (RAW) + JPEG Fine 0x1 = NEF (RAW) + JPEG Norm 0x2 = NEF (RAW) + JPEG Basic 0x3 = NEF (RAW) 0x4 = TIF (RGB) 0x5 = JPEG Fine 0x6 = JPEG Normal 0x7 = JPEG Basic
> 778 | CustomSettingsD3 | - | --> NikonCustom SettingsD3 Tags

## Nikon ShotInfoD3X Tags

These tags are extracted from encrypted data in images from the D3X with firmware 1.00.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 605 | ISO2 | int8u |
> 640 | ShutterCount | int32u |
> 779 | CustomSettingsD3X | - | --> NikonCustom SettingsD3 Tags

## Nikon ShotInfoD3S Tags

These tags are extracted from encrypted data in images from the D3S with firmware 1.00 and earlier.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 16 | ImageArea | int8u | 0 = FX (36x24) 1 = DX (24x16) 2 = 5:4 (30x24) 3 = 1.2x (30x20)
> 545 | ISO2 | int8u |
> 578 | ShutterCount | int32u |
> 718 | CustomSettingsD3S | - | --> NikonCustom SettingsD3 Tags

## Nikon ShotInfoD300a Tags

These tags are extracted from encrypted data in images from the D300 with firmware 1.00 and earlier.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 604 | ISO2 | int8u |
> 633 | ShutterCount | int32u |
> 721 | AFFineTuneAdj | int16u |
> 0x0 = 0 0x3a = +1 0x3b = +2 0x3c = +4 0x3d = +8 0x3e = +16 0xc2 = -16 0xc3 = -8 0xc4 = -4 0xc5 = -2 0xc6 = -1 0x103e = +17 0x10c2 = -17 0x203d = +9 |  | 0x203e = +18 0x20c2 = -18 0x20c3 = -9 0x303e = +19 0x30c2 = -19 0x403c = +5 0x403d = +10 0x403e = +20 0x40c2 = -20 0x40c3 = -10 0x40c4 = -5 0x603d = +11 0x60c3 = -11 0x803b = +3 |  | 0x803c = +6 0x803d = +12 0x80c3 = -12 0x80c4 = -6 0x80c5 = -3 0xa03d = +13 0xa0c3 = -13 0xc03c = +7 0xc03d = +14 0xc0c3 = -14 0xc0c4 = -7 0xe03d = +15 0xe0c3 = -15
> 790 | CustomSettingsD300 | - | --> NikonCustom SettingsD3 Tags

## Nikon ShotInfoD300b Tags

These tags are extracted from encrypted data in images from the D300 with firmware 1.10.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 613 | ISO2 | int8u |
> 644 | ShutterCount | int32u |
> 732 | AFFineTuneAdj | int16u | (firmware version 1.10B)
> 0x0 = 0 0x83e = +11 0x8c2 = -11 0x203c = +3 0x203d = +6 0x203e = +12 0x20c2 = -12 0x20c3 = -6 0x20c4 = -3 0x383e = +13 0x38c2 = -13 0x503d = +7 0x503e = +14 0x50c2 = -14 |  | 0x50c3 = -7 0x683e = +15 0x68c2 = -15 0x803a = +1 0x803b = +2 0x803c = +4 0x803d = +8 0x803e = +16 0x80c2 = -16 0x80c3 = -8 0x80c4 = -4 0x80c5 = -2 0x80c6 = -1 0x983e = +17 |  | 0x98c2 = -17 0xb03d = +9 0xb03e = +18 0xb0c2 = -18 0xb0c3 = -9 0xc83e = +19 0xc8c2 = -19 0xe03c = +5 0xe03d = +10 0xe03e = +20 0xe0c2 = -20 0xe0c3 = -10 0xe0c4 = -5
> (other versions)
> 0x0 = 0 0x43e = +13 0x4c2 = -13 0x183d = +7 0x183e = +14 0x18c2 = -14 0x18c3 = -7 0x2c3e = +15 0x2cc2 = -15 0x403a = +1 0x403b = +2 0x403c = +4 0x403d = +8 0x403e = +16 |  | 0x40c2 = -16 0x40c3 = -8 0x40c4 = -4 0x40c5 = -2 0x40c6 = -1 0x543e = +17 0x54c2 = -17 0x683d = +9 0x683e = +18 0x68c2 = -18 0x68c3 = -9 0x7c3e = +19 0x7cc2 = -19 0x903c = +5 |  | 0x903d = +10 0x903e = +20 0x90c2 = -20 0x90c3 = -10 0x90c4 = -5 0xb83d = +11 0xb8c3 = -11 0xe03b = +3 0xe03c = +6 0xe03d = +12 0xe0c3 = -12 0xe0c4 = -6 0xe0c5 = -3
> 802 | CustomSettingsD300 | - | --> NikonCustom SettingsD3 Tags

## Nikon ShotInfoD300S Tags

These tags are extracted from encrypted data in images from the D300S with firmware 1.00.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 613 | ISO2 | int8u |
> 646 | ShutterCount | int32u |
> 804 | CustomSettingsD300S | - | --> NikonCustom SettingsD3 Tags

## Nikon ShotInfoD700 Tags

These tags are extracted from encrypted data in images from the D700 with firmware 1.02f.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 613 | ISO2 | int8u |
> 647 | ShutterCount | int32u |
> 804 | CustomSettingsD700 | - | --> NikonCustom SettingsD700 Tags

## Nikon ShotInfoD800 Tags

These tags are extracted from encrypted data in images from the D800.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 1216 | RepeatingFlashOutputExternal | int8u |
> 1218 | RepeatingFlashRateExternal | int8u |
> 1219 | RepeatingFlashCountExternal | int8u |
> 1234 | FlashExposureComp2 | int8s | (includes the effect of flash bracketing)
> 1242 | RepeatingFlashRateBuilt-in | int8u |
> 1243 | RepeatingFlashCountBuilt-in | int8u |
> 1308 | SequenceNumber | int8u |
> 1531 | ShutterCount | int32u |
> 1772 | CustomSettingsD800 | - | --> NikonCustom SettingsD800 Tags

## Nikon ShotInfoD810 Tags

These tags are extracted from encrypted data in images from the D810.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 36 | BracketingOffset | no |
> 64 | CustomSettingsOffset | no |
> 132 | OrientationOffset | no |
> 464 | SecondarySlotFunction | int8u | [Mask 0x03] 0x0 = Overflow 0x2 = Backup 0x3 = NEF Primary + JPG Secondary
> 5974 | AEBracketingSteps | int8u | [Mask 0xff]
> 0x0 = AE Bracketing Disabled 0x20 = AE Bracketing Disabled 0x30 = AE Bracketing Disabled 0x40 = AE Bracketing Disabled 0x50 = AE Bracketing Disabled 0x81 = +3F0.3 0x82 = -3F0.3 0x83 = +2F0.3 0x84 = -2F0.3 0x85 = 3F0.3 0x86 = 5F0.3 0x87 = 7F0.3 0x88 = 9F0.3 0x91 = +3F0.5 0x92 = -3F0.5 0x93 = +2F0.5 0x94 = -2F0.5 0x95 = 3F0.5 0x96 = 5F0.5 0x97 = 7F0.5 0x98 = 9F0.5 0xa1 = +3F0.7 0xa2 = -3F0.7 0xa3 = +2F0.7 0xa4 = -2F0.7 |  | 0xa5 = 3F0.7 0xa6 = 5F0.7 0xa7 = 7F0.7 0xa8 = 9F0.7 0xb1 = +3F1 0xb2 = -3F1 0xb3 = +2F1 0xb4 = -2F1 0xb5 = 3F1 0xb6 = 5F1 0xb7 = 7F1 0xb8 = 9F1 0xc1 = +3F2 0xc2 = -3F2 0xc3 = +2F2 0xc4 = -2F2 0xc5 = 3F2 0xc6 = 5F2 0xd1 = +3F3 0xd2 = -3F3 0xd3 = +2F3 0xd4 = -2F3 0xd5 = 3F3 0xd6 = 5F3
> 5975 | WBBracketingSteps | int8u | [Mask 0xff]
> 0x0 = WB Bracketing Disabled 0x1 = b3F 1 0x2 = A3F 1 0x3 = b2F 1 0x4 = A2F 1 0x5 = 3F 1 0x6 = 5F 1 0x7 = 7F 1 0x8 = 9F 1 0x10 = 0F 2 0x11 = b3F 2 0x12 = A3F 2 0x13 = b2F 2 0x14 = A2F 2 |  | 0x15 = 3F 2 0x16 = 5F 2 0x17 = 7F 2 0x18 = 9F 2 0x20 = 0F 3 0x21 = b3F 3 0x22 = A3F 3 0x23 = b2F 3 0x24 = A2F 3 0x25 = 3F 3 0x26 = 5F 3 0x27 = 7F 3 0x28 = 9F 3
> 5982 | D810MeteringMode | int8u | [Mask 0x03] 0x0 = Matrix 0x1 = Center 0x2 = Spot 0x3 = Highlight
> 6236 | ISOAutoShutterTime | int8u | [Mask 0x3f]
> 0x0 = 1/4000 s 0x1 = 1/3200 s 0x2 = 1/2500 s 0x3 = 1/2000 s 0x4 = 1/1600 s 0x5 = 1/1250 s 0x6 = 1/1000 s 0x7 = 1/800 s 0x8 = 1/640 s 0x9 = 1/500 s 0xa = 1/400 s 0xb = 1/320 s 0xc = 1/250 s 0xd = 1/200 s 0xe = 1/160 s 0xf = 1/125 s 0x10 = 1/100 s 0x11 = 1/80 s 0x12 = 1/60 s |  | 0x13 = 1/50 s 0x14 = 1/40 s 0x15 = 1/30 s 0x16 = 1/15 s 0x17 = 1/8 s 0x18 = 1/4 s 0x19 = 1/2 s 0x1a = 1 s 0x1b = 2 s 0x1c = 4 s 0x1d = 8 s 0x1e = 15 s 0x1f = 30 s 0x20 = Auto (Slowest) 0x21 = Auto (Slower) 0x22 = Auto 0x23 = Auto (Faster) 0x24 = Auto (Fastest)
> 6237 | ISOAutoHiLimit | int8u | [Mask 0xff]
> 0x24 = ISO 200 0x26 = ISO 250 0x27 = ISO 280 0x28 = ISO 320 0x2a = ISO 400 0x2c = ISO 500 0x2d = ISO 560 0x2e = ISO 640 0x30 = ISO 800 0x32 = ISO 1000 0x33 = ISO 1100 0x34 = ISO 1250 0x36 = ISO 1600 0x38 = ISO 2000 0x39 = ISO 2200 0x3a = ISO 2500 0x3c = ISO 3200 0x3e = ISO 4000 0x3f = ISO 4500 0x40 = ISO 5000 0x42 = ISO 6400 |  | 0x44 = ISO 8000 0x45 = ISO 9000 0x46 = ISO 10000 0x48 = ISO 12800 0x4a = ISO 16000 0x4b = ISO 18000 0x4c = ISO 20000 0x4e = ISO 25600 0x50 = ISO 32000 0x51 = ISO 36000 0x52 = ISO 40000 0x54 = ISO 51200 0x56 = ISO Hi 0.3 0x57 = ISO Hi 0.5 0x58 = ISO Hi 0.7 0x5a = ISO Hi 1.0 0x60 = ISO Hi 2.0 0x66 = ISO Hi 3.0 0x6c = ISO Hi 4.0 0x72 = ISO Hi 5.0
> 6315 | CustomSettingsD810 | - | --> NikonCustom SettingsD810 Tags (actual offset determined by CustomSettingsOffset)
> 14068 | RollAngle | fixed32u | (converted to degrees of clockwise camera roll)
> 14072 | PitchAngle | fixed32u | (converted to degrees of upward camera tilt)
> 14076 | YawAngle | fixed32u | (the camera yaw angle when shooting in portrait orientation)

## Nikon ShotInfoD850 Tags

These tags are extracted from encrypted data in images from the D850.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 88 | CustomSettingsOffset | no |
> 1937 | PhotoShootingMenuBankImageArea | int8u | [Mask 0x07] 0x0 = FX (36x24) 0x1 = DX (24x16) 0x2 = 5:4 (30x24) 0x3 = 1.2x (30x20) 0x4 = 1:1 (24x24)
> 4029 | PhotoShootingMenuBank | int8u | [Mask 0x03] 0x0 = A 0x1 = B 0x2 = C 0x3 = D
> 4031 | PrimarySlot | int8u | [Mask 0x80] 0x0 = XQD Card 0x80 = SD Card
> 4152 | CustomSettingsD850 | - | --> NikonCustom SettingsD850 Tags

## Nikon ShotInfoD5000 Tags

These tags are extracted from encrypted data in images from the D5000 with firmware 1.00.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 693 | ISO2 | int8u |
> 726 | ShutterCount | int32u |
> 888 | CustomSettingsD5000 | - | --> NikonCustom SettingsD5000 Tags

## Nikon ShotInfoD5100 Tags

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 801 | ShutterCount | int32u |
> 1031 | CustomSettingsD5100 | - | --> NikonCustom SettingsD5100 Tags

## Nikon ShotInfoD5200 Tags

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 3032 | ShutterCount | int32u |
> 3285 | CustomSettingsD5200 | - | --> NikonCustom SettingsD5200 Tags

## Nikon ShotInfoD7000 Tags

These tags are extracted from encrypted data in images from the D7000 with firmware 1.01b.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 800 | ShutterCount | int32u |
> 1028 | CustomSettingsD7000 | - | --> NikonCustom SettingsD7000 Tags

## Nikon ShotInfoD4 Tags

These tags are extracted from encrypted data in images from the D4.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 1873 | CustomSettingsD4 | - | --> NikonCustom SettingsD4 Tags

## Nikon ShotInfoD4S Tags

These tags are extracted from encrypted data in images from the D4S.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 464 | SecondarySlotFunction | int8u | [Mask 0x03] 0x0 = Overflow 0x2 = Backup 0x3 = NEF Primary + JPG Secondary
> 5964 | AEBracketingSteps | int8u | [Mask 0xff]
> 0x0 = AE Bracketing Disabled 0x20 = AE Bracketing Disabled 0x30 = AE Bracketing Disabled 0x40 = AE Bracketing Disabled 0x50 = AE Bracketing Disabled 0x81 = +3F0.3 0x82 = -3F0.3 0x83 = +2F0.3 0x84 = -2F0.3 0x85 = 3F0.3 0x86 = 5F0.3 0x87 = 7F0.3 0x88 = 9F0.3 0x91 = +3F0.5 0x92 = -3F0.5 0x93 = +2F0.5 0x94 = -2F0.5 0x95 = 3F0.5 0x96 = 5F0.5 0x97 = 7F0.5 0x98 = 9F0.5 0xa1 = +3F0.7 0xa2 = -3F0.7 0xa3 = +2F0.7 0xa4 = -2F0.7 |  | 0xa5 = 3F0.7 0xa6 = 5F0.7 0xa7 = 7F0.7 0xa8 = 9F0.7 0xb1 = +3F1 0xb2 = -3F1 0xb3 = +2F1 0xb4 = -2F1 0xb5 = 3F1 0xb6 = 5F1 0xb7 = 7F1 0xb8 = 9F1 0xc1 = +3F2 0xc2 = -3F2 0xc3 = +2F2 0xc4 = -2F2 0xc5 = 3F2 0xc6 = 5F2 0xd1 = +3F3 0xd2 = -3F3 0xd3 = +2F3 0xd4 = -2F3 0xd5 = 3F3 0xd6 = 5F3
> 5965 | WBBracketingSteps | int8u | [Mask 0xff]
> 0x0 = WB Bracketing Disabled 0x1 = b3F 1 0x2 = A3F 1 0x3 = b2F 1 0x4 = A2F 1 0x5 = 3F 1 0x6 = 5F 1 0x7 = 7F 1 0x8 = 9F 1 0x10 = 0F 2 0x11 = b3F 2 0x12 = A3F 2 0x13 = b2F 2 0x14 = A2F 2 |  | 0x15 = 3F 2 0x16 = 5F 2 0x17 = 7F 2 0x18 = 9F 2 0x20 = 0F 3 0x21 = b3F 3 0x22 = A3F 3 0x23 = b2F 3 0x24 = A2F 3 0x25 = 3F 3 0x26 = 5F 3 0x27 = 7F 3 0x28 = 9F 3
> 6221 | ReleaseMode | int8u | [Mask 0xff]
> 0x0 = Single Frame 0x1 = Continuous High Speed 0x3 = Continuous Low Speed 0x4 = Timer 0x20 = Mirror-Up 0x40 = Quiet
> 6301 | CustomSettingsD4S | - | --> NikonCustom SettingsD4 Tags (firmware version 1.00)
> 6338 | MultiSelectorLiveViewMode | int8u | [Mask 0xc0] 0x0 = Reset 0x40 = Zoom 0xc0 = None
> 6378 | ISOAutoShutterTime | int8u | [Mask 0x3f]
> 0x0 = 1/4000 s 0x1 = 1/3200 s 0x2 = 1/2500 s 0x3 = 1/2000 s 0x4 = 1/1600 s 0x5 = 1/1250 s 0x6 = 1/1000 s 0x7 = 1/800 s 0x8 = 1/640 s 0x9 = 1/500 s 0xa = 1/400 s 0xb = 1/320 s 0xc = 1/250 s 0xd = 1/200 s 0xe = 1/160 s 0xf = 1/125 s 0x10 = 1/100 s 0x11 = 1/80 s 0x12 = 1/60 s |  | 0x13 = 1/50 s 0x14 = 1/40 s 0x15 = 1/30 s 0x16 = 1/15 s 0x17 = 1/8 s 0x18 = 1/4 s 0x19 = 1/2 s 0x1a = 1 s 0x1b = 2 s 0x1c = 4 s 0x1d = 8 s 0x1e = 15 s 0x1f = 30 s 0x20 = Auto (Slowest) 0x21 = Auto (Slower) 0x22 = Auto 0x23 = Auto (Faster) 0x24 = Auto (Fastest)
> 6379 | ISOAutoHiLimit | int8u | [Mask 0xff]
> 0x24 = ISO 200 0x26 = ISO 250 0x27 = ISO 280 0x28 = ISO 320 0x2a = ISO 400 0x2c = ISO 500 0x2d = ISO 560 0x2e = ISO 640 0x30 = ISO 800 0x32 = ISO 1000 0x33 = ISO 1100 0x34 = ISO 1250 0x36 = ISO 1600 0x38 = ISO 2000 0x39 = ISO 2200 0x3a = ISO 2500 0x3c = ISO 3200 0x3e = ISO 4000 0x3f = ISO 4500 0x40 = ISO 5000 0x42 = ISO 6400 |  | 0x44 = ISO 8000 0x45 = ISO 9000 0x46 = ISO 10000 0x48 = ISO 12800 0x4a = ISO 16000 0x4b = ISO 18000 0x4c = ISO 20000 0x4e = ISO 25600 0x50 = ISO 32000 0x51 = ISO 36000 0x52 = ISO 40000 0x54 = ISO 51200 0x56 = ISO Hi 0.3 0x57 = ISO Hi 0.5 0x58 = ISO Hi 0.7 0x5a = ISO Hi 1.0 0x60 = ISO Hi 2.0 0x66 = ISO Hi 3.0 0x6c = ISO Hi 4.0 0x72 = ISO Hi 5.0
> 6461 | CustomSettingsD4S | - | --> NikonCustom SettingsD4 Tags (firmware version 1.01)
> 13579 | RollAngle | fixed32u | (converted to degrees of clockwise camera roll)
> 13583 | PitchAngle | fixed32u | (converted to degrees of upward camera tilt)
> 13587 | YawAngle | fixed32u | (the camera yaw angle when shooting in portrait orientation)
> 13971 | Rotation | int8u | [Mask 0x30] 0x0 = Horizontal 0x10 = Rotate 270 CW 0x20 = Rotate 90 CW 0x30 = Rotate 180

## Nikon ShotInfoD500 Tags

These tags are extracted from encrypted data in images from the D5 and D500.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 16 | RotationInfoOffset | no |
> 20 | JPGInfoOffset | no |
> 44 | BracketingInfoOffset | no |
> 80 | ShootingMenuOffset | no |
> 88 | CustomSettingsOffset | no |
> 160 | OrientationOffset | no |
> 202 | Rotation | int8u | [Mask 0x03] 0x0 = Horizontal 0x1 = Rotate 270 CW 0x2 = Rotate 90 CW 0x3 = Rotate 180
> 1506 | FlickerReductionIndicator | int8u | [Mask 0x01] 0x0 = On 0x1 = Off
> 2004 | JPGCompression | int8u | [Mask 0x01] 0x0 = Size Priority 0x1 = Optimal Quality
> 2171 | AEBracketingSteps | int8u | [Mask 0xff]
> 0x0 = AE Bracketing Disabled 0x20 = AE Bracketing Disabled 0x30 = AE Bracketing Disabled 0x40 = AE Bracketing Disabled 0x50 = AE Bracketing Disabled 0x81 = +3F0.3 0x82 = -3F0.3 0x83 = +2F0.3 0x84 = -2F0.3 0x85 = 3F0.3 0x86 = 5F0.3 0x87 = 7F0.3 0x88 = 9F0.3 0x91 = +3F0.5 0x92 = -3F0.5 0x93 = +2F0.5 0x94 = -2F0.5 0x95 = 3F0.5 0x96 = 5F0.5 0x97 = 7F0.5 0x98 = 9F0.5 0xa1 = +3F0.7 0xa2 = -3F0.7 0xa3 = +2F0.7 0xa4 = -2F0.7 |  | 0xa5 = 3F0.7 0xa6 = 5F0.7 0xa7 = 7F0.7 0xa8 = 9F0.7 0xb1 = +3F1 0xb2 = -3F1 0xb3 = +2F1 0xb4 = -2F1 0xb5 = 3F1 0xb6 = 5F1 0xb7 = 7F1 0xb8 = 9F1 0xc1 = +3F2 0xc2 = -3F2 0xc3 = +2F2 0xc4 = -2F2 0xc5 = 3F2 0xc6 = 5F2 0xd1 = +3F3 0xd2 = -3F3 0xd3 = +2F3 0xd4 = -2F3 0xd5 = 3F3 0xd6 = 5F3
> 2172 | WBBracketingSteps | int8u | [Mask 0xff]
> 0x0 = WB Bracketing Disabled 0x1 = b3F 1 0x2 = A3F 1 0x3 = b2F 1 0x4 = A2F 1 0x5 = 3F 1 0x6 = 5F 1 0x7 = 7F 1 0x8 = 9F 1 0x10 = 0F 2 0x11 = b3F 2 0x12 = A3F 2 0x13 = b2F 2 0x14 = A2F 2 |  | 0x15 = 3F 2 0x16 = 5F 2 0x17 = 7F 2 0x18 = 9F 2 0x20 = 0F 3 0x21 = b3F 3 0x22 = A3F 3 0x23 = b2F 3 0x24 = A2F 3 0x25 = 3F 3 0x26 = 5F 3 0x27 = 7F 3 0x28 = 9F 3
> 2179 | ADLBracketingStep | int8u | [Mask 0xf0]
> 0x0 = Off 0x10 = Low 0x20 = Normal |  | 0x30 = High 0x40 = Extra High 0x80 = Auto
> 2180 | ADLBracketingType | int8u | [Mask 0x0f] 0x0 = Off 0x1 = 2 Shots 0x2 = 3 Shots 0x3 = 4 Shots 0x4 = 5 Shots
> 3709 | PhotoShootingMenuBank | int8u | [Mask 0x03] 0x0 = A 0x1 = B 0x2 = C 0x3 = D
> 3711 | PrimarySlot | int8u | (D500 only) [Mask 0x80] 0x0 = XQD Card 0x80 = SD Card
> 3713 | ISOAutoShutterTime | int8u | [Mask 0x3f]
> 0x0 = 1/4000 s 0x1 = 1/3200 s 0x2 = 1/2500 s 0x3 = 1/2000 s 0x4 = 1/1600 s 0x5 = 1/1250 s 0x6 = 1/1000 s 0x7 = 1/800 s 0x8 = 1/640 s 0x9 = 1/500 s 0xa = 1/400 s 0xb = 1/320 s 0xc = 1/250 s 0xd = 1/200 s 0xe = 1/160 s 0xf = 1/125 s 0x10 = 1/100 s 0x11 = 1/80 s 0x12 = 1/60 s |  | 0x13 = 1/50 s 0x14 = 1/40 s 0x15 = 1/30 s 0x16 = 1/15 s 0x17 = 1/8 s 0x18 = 1/4 s 0x19 = 1/2 s 0x1a = 1 s 0x1b = 2 s 0x1c = 4 s 0x1d = 8 s 0x1e = 15 s 0x1f = 30 s 0x20 = Auto (Slowest) 0x21 = Auto (Slower) 0x22 = Auto 0x23 = Auto (Faster) 0x24 = Auto (Fastest)
> 3714 | ISOAutoHiLimit | int8u | [Mask 0xff]
> 0x24 = ISO 200 0x26 = ISO 250 0x27 = ISO 280 0x28 = ISO 320 0x2a = ISO 400 0x2c = ISO 500 0x2d = ISO 560 0x2e = ISO 640 0x30 = ISO 800 0x32 = ISO 1000 0x33 = ISO 1100 0x34 = ISO 1250 0x36 = ISO 1600 0x38 = ISO 2000 0x39 = ISO 2200 0x3a = ISO 2500 0x3c = ISO 3200 0x3e = ISO 4000 0x3f = ISO 4500 0x40 = ISO 5000 0x42 = ISO 6400 |  | 0x44 = ISO 8000 0x45 = ISO 9000 0x46 = ISO 10000 0x48 = ISO 12800 0x4a = ISO 16000 0x4b = ISO 18000 0x4c = ISO 20000 0x4e = ISO 25600 0x50 = ISO 32000 0x51 = ISO 36000 0x52 = ISO 40000 0x54 = ISO 51200 0x56 = ISO Hi 0.3 0x57 = ISO Hi 0.5 0x58 = ISO Hi 0.7 0x5a = ISO Hi 1.0 0x60 = ISO Hi 2.0 0x66 = ISO Hi 3.0 0x6c = ISO Hi 4.0 0x72 = ISO Hi 5.0
> 3716 | FlickerReduction | int8u | [Mask 0x20] 0x0 = Enable 0x20 = Disable
> 3716.1 | PhotoShootingMenuBankImageArea | int8u | [Mask 0x07] 0x0 = FX (36x24) 0x1 = DX (24x16) 0x2 = 5:4 (30x24) 0x3 = 1.2x (30x20) 0x4 = 1.3x (18x12)
> 3819 | CustomSettingsD5 CustomSettingsD500 | - - | --> NikonCustom SettingsD5 Tags --> NikonCustom SettingsD500 Tags
> 11300 | RollAngle | fixed32u | (converted to degrees of clockwise camera roll)
> 11304 | PitchAngle | fixed32u | (converted to degrees of upward camera tilt)
> 11308 | YawAngle | fixed32u | (the camera yaw angle when shooting in portrait orientation)

## Nikon ShotInfoD610 Tags

These tags are extracted from encrypted data in images from the D610.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 1999 | CustomSettingsD610 | - | --> NikonCustom SettingsD610 Tags

## Nikon ShotInfo Tags

This information is encrypted for ShotInfoVersion 02xx, and some tags are only valid for specific models.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShotInfoVersion | no |
> 4 | FirmwareVersion | no |
> 16 | DistortionControl | int8u | (P6000) 0 = Off 1 = On
> 102 | VR_0x66? | int8u | (D2X, D2Xs (unverified)) 0 = Off 1 = On (normal) 2 = On (active)
> 106 | ShutterCount | int32u | (D2X, D2Xs)
> 110 | DeletedImageCount | int32u | (D2X, D2Xs)
> 117 | VibrationReduction | int8u | (D200) 0 = Off 1 = On (1) 2 = On (2) 3 = On (3)
> 130 | VibrationReduction | int8u | (D2X, D2Xs) 0 = Off 1 = On
> 343 | ShutterCount | undef[2] | (D50)
> 430 | VibrationReduction | int8u | (D50) 0x0 = n/a 0xc = Off 0xf = On
> 589 | ShutterCount | int32u | (D60)

## Nikon ColorBalance1 Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | WB_RBGGLevels | int16u[4]! |

## Nikon ColorBalance2 Tags

This information is encrypted for most camera models.

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | WB_RGGBLevels | int16u[4]! |

## Nikon ColorBalance3 Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | WB_RGBGLevels | int16u[4]! |

## Nikon ColorBalance4 Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | WB_GRBGLevels | int16u[4]! |

## Nikon ColorBalanceUnknown Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ColorBalanceVersion | undef[4] |

## Nikon LensData00 Tags

This structure is used by the D100, and D1X with firmware version 1.1.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensDataVersion | no |
> 6 | LensIDNumber | int8u | (see LensID values below)
> 7 | LensFStops | int8u |
> 8 | MinFocalLength | int8u |
> 9 | MaxFocalLength | int8u |
> 10 | MaxApertureAtMinFocal | int8u |
> 11 | MaxApertureAtMaxFocal | int8u |
> 12 | MCUVersion | int8u |

## Nikon LensData01 Tags

Nikon encrypts the LensData information below if LensDataVersion is 0201 or higher, but the decryption algorithm is known so the information can be extracted.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensDataVersion | no |
> 4 | ExitPupilPosition | int8u |
> 5 | AFAperture | int8u |
> 8 | FocusPosition | int8u |
> 9 | FocusDistance | int8u | (this focus distance is approximate, and not very accurate for some lenses)
> 10 | FocalLength | int8u |
> 11 | LensIDNumber | int8u | (see LensID values below)
> 12 | LensFStops | int8u |
> 13 | MinFocalLength | int8u |
> 14 | MaxFocalLength | int8u |
> 15 | MaxApertureAtMinFocal | int8u |
> 16 | MaxApertureAtMaxFocal | int8u |
> 17 | MCUVersion | int8u |
> 18 | EffectiveMaxAperture | int8u |

## Nikon LensData0204 Tags

Nikon encrypts the LensData information below if LensDataVersion is 0201 or higher, but the decryption algorithm is known so the information can be extracted.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensDataVersion | no |
> 4 | ExitPupilPosition | int8u |
> 5 | AFAperture | int8u |
> 8 | FocusPosition | int8u |
> 10 | FocusDistance | int8u | (this focus distance is approximate, and not very accurate for some lenses)
> 11 | FocalLength | int8u |
> 12 | LensIDNumber | int8u | (see LensID values below)
> 13 | LensFStops | int8u |
> 14 | MinFocalLength | int8u |
> 15 | MaxFocalLength | int8u |
> 16 | MaxApertureAtMinFocal | int8u |
> 17 | MaxApertureAtMaxFocal | int8u |
> 18 | MCUVersion | int8u |
> 19 | EffectiveMaxAperture | int8u |

## Nikon LensData0400 Tags

Tags extracted from the encrypted lens data of Nikon 1 models.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensDataVersion | no |
> 394 | LensModel | string[64] |

## Nikon LensDataUnknown Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensDataVersion | no |

## Nikon FlashInfo0100 Tags

These tags are used by the D2H, D2Hs, D2X, D2Xs, D50, D70, D70s, D80 and D200.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FlashInfoVersion | no |
> 4 | FlashSource | int8u | 0 = None 1 = External 2 = Internal
> 6 | ExternalFlashFirmware | int8u[2] | --> Nikon FlashFirmware Values
> 8 | ExternalFlashFlags | int8u | 0x0 = (none) Bit 0 = Fired Bit 2 = Bounce Flash Bit 4 = Wide Flash Adapter Bit 5 = Dome Diffuser
> 9.1 | FlashCommanderMode | int8u | [Mask 0x80] 0x0 = Off 0x80 = On
> 9.2 | FlashControlMode | int8u | [Mask 0x7f] --> Nikon FlashControlMode Values
> 10 | FlashOutput FlashCompensation | int8u int8s |
> 11 | FlashFocalLength | int8u |
> 12 | RepeatingFlashRate | int8u |
> 13 | RepeatingFlashCount | int8u |
> 14 | FlashGNDistance | int8u | --> Nikon FlashGNDistance Values
> 15 | FlashGroupAControlMode | int8u | [Mask 0x0f] --> Nikon FlashControlMode Values
> 16 | FlashGroupBControlMode | int8u | [Mask 0x0f] --> Nikon FlashControlMode Values
> 17 | FlashGroupAOutput FlashGroupACompensation | int8u int8s |
> 18 | FlashGroupBOutput FlashGroupBCompensation | int8u int8s |

## Nikon FlashFirmware Values

> Value | FlashFirmware | Value | FlashFirmware
> --- | --- | --- | ---
> '0 0' | = n/a | '4 1' | = 4.01 (SB-400)
> '1 1' | = 1.01 (SB-800 or Metz 58 AF-1) | '4 2' | = 4.02 (SB-400)
> '1 3' | = 1.03 (SB-800) | '4 4' | = 4.04 (SB-400)
> '2 1' | = 2.01 (SB-800) | '5 1' | = 5.01 (SB-900)
> '2 4' | = 2.04 (SB-600) | '5 2' | = 5.02 (SB-900)
> '2 5' | = 2.05 (SB-600) | '6 1' | = 6.01 (SB-700)
> '3 1' | = 3.01 (SU-800 Remote Commander) | '7 1' | = 7.01 (SB-910)

## Nikon FlashControlMode Values

> Value | FlashControlMode | Value | FlashControlMode | Value | FlashControlMode
> --- | --- | --- | --- | --- | ---
> 0x0 | = Off | 0x3 | = Auto Aperture | 0x6 | = Manual
> 0x1 | = iTTL-BL | 0x4 | = Automatic | 0x7 | = Repeating Flash
> 0x2 | = iTTL | 0x5 | = GN (distance priority) |  |

## Nikon FlashGNDistance Values

> Value | FlashGNDistance | Value | FlashGNDistance | Value | FlashGNDistance
> --- | --- | --- | --- | --- | ---
> 0 | = 0 | 13 | = 1.4 m | 26 | = 6.3 m
> 1 | = 0.1 m | 14 | = 1.6 m | 27 | = 7.1 m
> 2 | = 0.2 m | 15 | = 1.8 m | 28 | = 8.0 m
> 3 | = 0.3 m | 16 | = 2.0 m | 29 | = 9.0 m
> 4 | = 0.4 m | 17 | = 2.2 m | 30 | = 10.0 m
> 5 | = 0.5 m | 18 | = 2.5 m | 31 | = 11.0 m
> 6 | = 0.6 m | 19 | = 2.8 m | 32 | = 13.0 m
> 7 | = 0.7 m | 20 | = 3.2 m | 33 | = 14.0 m
> 8 | = 0.8 m | 21 | = 3.6 m | 34 | = 16.0 m
> 9 | = 0.9 m | 22 | = 4.0 m | 35 | = 18.0 m
> 10 | = 1.0 m | 23 | = 4.5 m | 36 | = 20.0 m
> 11 | = 1.1 m | 24 | = 5.0 m | 255 | = n/a
> 12 | = 1.3 m | 25 | = 5.6 m |  |

## Nikon FlashInfo0102 Tags

These tags are used by the D3 (firmware 1.x), D40, D40X, D60 and D300 (firmware 1.00).

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FlashInfoVersion | no |
> 4 | FlashSource | int8u | 0 = None 1 = External 2 = Internal
> 6 | ExternalFlashFirmware | int8u[2] | --> Nikon FlashFirmware Values
> 8 | ExternalFlashFlags | int8u | Bit 0 = Fired Bit 2 = Bounce Flash Bit 4 = Wide Flash Adapter Bit 5 = Dome Diffuser
> 9.1 | FlashCommanderMode | int8u | [Mask 0x80] 0x0 = Off 0x80 = On
> 9.2 | FlashControlMode | int8u | [Mask 0x7f] --> Nikon FlashControlMode Values
> 10 | FlashOutput FlashCompensation | int8u int8s |
> 12 | FlashFocalLength | int8u |
> 13 | RepeatingFlashRate | int8u |
> 14 | RepeatingFlashCount | int8u |
> 15 | FlashGNDistance | int8u | --> Nikon FlashGNDistance Values
> 16.1 | FlashGroupAControlMode | int8u | [Mask 0x0f] --> Nikon FlashControlMode Values (note: group A tags may apply to the built-in flash settings for some models)
> 17.1 | FlashGroupBControlMode | int8u | [Mask 0xf0] --> Nikon FlashControlMode Values (note: group B tags may apply to group A settings for some models)
> 17.2 | FlashGroupCControlMode | int8u | [Mask 0x0f] --> Nikon FlashControlMode Values (note: group C tags may apply to group B settings for some models)
> 18 | FlashGroupAOutput FlashGroupACompensation | int8u int8s |
> 19 | FlashGroupBOutput FlashGroupBCompensation | int8u int8s |
> 20 | FlashGroupCOutput FlashGroupCCompensation | int8u int8s |

## Nikon FlashInfo0103 Tags

These tags are used by the D3 (firmware 2.x), D3X, D3S, D4, D90, D300 (firmware 1.10), D300S, D600, D700, D800, D3000, D3100, D3200, D5000, D5100, D5200, D7000.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FlashInfoVersion | no |
> 4 | FlashSource | int8u | 0 = None 1 = External 2 = Internal
> 6 | ExternalFlashFirmware | int8u[2] | --> Nikon FlashFirmware Values
> 8 | ExternalFlashFlags | int8u | Bit 0 = Fired Bit 2 = Bounce Flash Bit 4 = Wide Flash Adapter Bit 5 = Dome Diffuser
> 9.1 | FlashCommanderMode | int8u | [Mask 0x80] 0x0 = Off 0x80 = On
> 9.2 | FlashControlMode | int8u | [Mask 0x7f] --> Nikon FlashControlMode Values
> 10 | FlashOutput FlashCompensation | int8u int8s |
> 12 | FlashFocalLength | int8u |
> 13 | RepeatingFlashRate | int8u |
> 14 | RepeatingFlashCount | int8u |
> 15 | FlashGNDistance | int8u | --> Nikon FlashGNDistance Values
> 16 | FlashColorFilter | int8u |
> 0 = None 1 = FL-GL1 2 = FL-GL2 |  | 9 = TN-A1 10 = TN-A2 65 = Red |  | 66 = Blue 67 = Yellow 68 = Amber
> 17.1 | FlashGroupAControlMode | int8u | [Mask 0x0f] --> Nikon FlashControlMode Values (note: group A tags may apply to the built-in flash settings for some models)
> 18.1 | FlashGroupBControlMode | int8u | [Mask 0xf0] --> Nikon FlashControlMode Values (note: group B tags may apply to group A settings for some models)
> 18.2 | FlashGroupCControlMode | int8u | [Mask 0x0f] --> Nikon FlashControlMode Values (note: group C tags may apply to group B settings for some models)
> 19 | FlashGroupAOutput FlashGroupACompensation | int8u int8s |
> 20 | FlashGroupBOutput FlashGroupBCompensation | int8u int8s |
> 21 | FlashGroupCOutput FlashGroupCCompensation | int8u int8s |
> 27 | ExternalFlashCompensation | int8s |
> 29 | FlashExposureComp3 | int8s | (does not include the effect of flash bracketing)
> 39 | FlashExposureComp4 | int8s | (includes the effect of flash bracketing. Valid for repeating flash)

## Nikon FlashInfo0107 Tags

These tags are used by the D4S, D750, D810, D5500, D7200 (FlashInfoVersion 0107) and the D5, D500 and D3400 (FlashInfoVersion 0108).

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FlashInfoVersion | no |
> 4 | FlashSource | int8u | 0 = None 1 = External 2 = Internal
> 6 | ExternalFlashFirmware | int8u[2] | --> Nikon FlashFirmware Values
> 8.1 | ExternalFlashZoomOverride | int8u | (indicates that the user has overridden the flash zoom distance) [Mask 0x80] 0x0 = No 0x80 = Yes
> 8.2 | ExternalFlashStatus | int8u | [Mask 0x01] 0x0 = Flash Not Attached 0x1 = Flash Attached
> 9.1 | ExternalFlashReadyState | int8u | [Mask 0x07] 0x0 = n/a 0x1 = Ready 0x6 = Not Ready
> 10 | FlashCompensation | int8s |
> 12 | FlashFocalLength | int8u | (only valid if flash pattern is "Standard Illumination")
> 13 | RepeatingFlashRate | int8u |
> 14 | RepeatingFlashCount | int8u |
> 15 | FlashGNDistance | int8u | --> Nikon FlashGNDistance Values

## Nikon FlashInfoUnknown Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FlashInfoVersion | no |

## Nikon MultiExposure Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | MultiExposureVersion | no |
> 1 | MultiExposureMode | int32u | 0 = Off 1 = Multiple Exposure 2 = Image Overlay 3 = HDR
> 2 | MultiExposureShots | int32u |
> 3 | MultiExposureAutoGain | int32u | 0 = Off 1 = On

## Nikon AFInfo2 Tags

These tags are written by Nikon DSLR's which have the live view feature.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | AFInfo2Version | no |
> 4 | ContrastDetectAF | int8u | (this is Off for the hybrid AF used in Nikon 1 models) 0 = Off 1 = On
> 5 | AFAreaMode | int8u | (ContrastDetectAF Off)
> 0 = Single Area 1 = Dynamic Area 2 = Dynamic Area (closest subject) 3 = Group Dynamic 4 = Dynamic Area (9 points) 5 = Dynamic Area (21 points) 6 = Dynamic Area (51 points) 7 = Dynamic Area (51 points, 3D-tracking) 8 = Auto-area 9 = Dynamic Area (3D-tracking) 10 = Single Area (wide) 11 = Dynamic Area (wide) 12 = Dynamic Area (wide, 3D-tracking) 13 = Group Area 14 = Dynamic Area (25 points) 15 = Dynamic Area (72 points) 16 = Group Area (HL) 17 = Group Area (VL) 128 = Single 129 = Auto (41 points) 130 = Subject Tracking (41 points) 131 = Face Priority (41 points)
> (ContrastDetectAF On)
> 0 = Contrast-detect 1 = Contrast-detect (normal area) 2 = Contrast-detect (wide area) 3 = Contrast-detect (face priority) 4 = Contrast-detect (subject tracking) 128 = Single 129 = Auto (41 points) 130 = Subject Tracking (41 points) 131 = Face Priority (41 points)
> 6 | PhaseDetectAF | int8u | (PrimaryAFPoint and AFPointsUsed below are only valid when this is On)
> 0 = Off 1 = On (51-point) 2 = On (11-point) 3 = On (39-point) |  | 4 = On (73-point) 5 = On (5) 6 = On (105-point) 7 = On (153-point)
> 7 | PrimaryAFPoint | int8u | (models with 51-point AF: D3, D3S, D3X, D300, D300S, D700 and D800)
> 0 = (none) 1 = C6 (Center) 2 = B6 3 = A5 4 = D6 5 = E5 6 = C7 7 = B7 8 = A6 9 = D7 10 = E6 |  | 11 = C5 12 = B5 13 = A4 14 = D5 15 = E4 16 = C8 17 = B8 18 = A7 19 = D8 20 = E7 21 = C9 |  | 22 = B9 23 = A8 24 = D9 25 = E8 26 = C10 27 = B10 28 = A9 29 = D10 30 = E9 31 = C11 32 = B11 |  | 33 = D11 34 = C4 35 = B4 36 = A3 37 = D4 38 = E3 39 = C3 40 = B3 41 = A2 42 = D3 43 = E2 |  | 44 = C2 45 = B2 46 = A1 47 = D2 48 = E1 49 = C1 50 = B1 51 = D1
> (models with 11-point AF: D90, D3000, D3100, D5000 and D5100)
> 0 = (none) 1 = Center 2 = Top 3 = Bottom 4 = Mid-left 5 = Upper-left |  | 6 = Lower-left 7 = Far Left 8 = Mid-right 9 = Upper-right 10 = Lower-right 11 = Far Right
> (models with 39-point AF: D600 and D7000)
> 0 = (none) 1 = C6 (Center) 2 = B6 3 = A2 4 = D6 5 = E2 6 = C7 7 = B7 |  | 8 = A3 9 = D7 10 = E3 11 = C5 12 = B5 13 = A1 14 = D5 15 = E1 |  | 16 = C8 17 = B8 18 = D8 19 = C9 20 = B9 21 = D9 22 = C10 23 = B10 |  | 24 = D10 25 = C11 26 = B11 27 = D11 28 = C4 29 = B4 30 = D4 31 = C3 |  | 32 = B3 33 = D3 34 = C2 35 = B2 36 = D2 37 = C1 38 = B1 39 = D1
> (Nikon 1 models with older 135-point AF and 73-point phase-detect AF)
> 0 = (none) 1 = E8 (Center) 2 = D8 3 = C8 4 = B8 5 = A8 6 = F8 7 = G8 8 = H8 9 = I8 10 = E9 11 = D9 12 = C9 13 = B9 14 = A9 15 = F9 16 = G9 17 = H9 18 = I9 19 = E7 20 = D7 21 = C7 22 = B7 23 = A7 24 = F7 25 = G7 26 = H7 27 = I7 |  | 28 = E10 29 = D10 30 = C10 31 = B10 32 = A10 33 = F10 34 = G10 35 = H10 36 = I10 37 = E11 38 = D11 39 = C11 40 = B11 41 = A11 42 = F11 43 = G11 44 = H11 45 = I11 46 = E12 47 = D12 48 = C12 49 = B12 50 = A12 51 = F12 52 = G12 53 = H12 54 = I12 55 = E13 |  | 56 = D13 57 = C13 58 = B13 59 = A13 60 = F13 61 = G13 62 = H13 63 = I13 64 = E14 65 = D14 66 = C14 67 = B14 68 = A14 69 = F14 70 = G14 71 = H14 72 = I14 73 = E15 74 = D15 75 = C15 76 = B15 77 = A15 78 = F15 79 = G15 80 = H15 81 = I15 82 = E6 83 = D6 |  | 84 = C6 85 = B6 86 = A6 87 = F6 88 = G6 89 = H6 90 = I6 91 = E5 92 = D5 93 = C5 94 = B5 95 = A5 96 = F5 97 = G5 98 = H5 99 = I5 100 = E4 101 = D4 102 = C4 103 = B4 104 = A4 105 = F4 106 = G4 107 = H4 108 = I4 109 = E3 110 = D3 111 = C3 |  | 112 = B3 113 = A3 114 = F3 115 = G3 116 = H3 117 = I3 118 = E2 119 = D2 120 = C2 121 = B2 122 = A2 123 = F2 124 = G2 125 = H2 126 = I2 127 = E1 128 = D1 129 = C1 130 = B1 131 = A1 132 = F1 133 = G1 134 = H1 135 = I1
> (Nikon 1 models with newer 135-point AF and 73-point phase-detect AF -- 9 rows (B-J) and 15 columns (1-15), inside a grid of 11 rows by 15 columns. The points are numbered sequentially, with F8 at the center) 0 = (none) 82 = F8 (Center) (Nikon 1 models with 171-point AF and 105-point phase-detect AF -- 9 rows (B-J) and 19 columns (2-20), inside a grid of 11 rows by 21 columns. The points are numbered sequentially, with F11 at the center) 0 = (none) 115 = F11 (Center) (Nikon models with 153-point AF -- 9 rows (A-I) and 17 columns (1-17))
> 0 = (none) 1 = E9 (Center) 2 = D9 3 = C9 4 = B9 5 = A9 6 = F9 7 = G9 8 = H9 9 = I9 10 = E10 11 = D10 12 = C10 13 = B10 14 = A10 15 = F10 16 = G10 17 = H10 18 = I10 19 = E11 20 = D11 21 = C11 22 = B11 23 = A11 24 = F11 25 = G11 26 = H11 27 = I11 28 = E8 29 = D8 30 = C8 |  | 31 = B8 32 = A8 33 = F8 34 = G8 35 = H8 36 = I8 37 = E7 38 = D7 39 = C7 40 = B7 41 = A7 42 = F7 43 = G7 44 = H7 45 = I7 46 = E12 47 = D12 48 = C12 49 = B12 50 = A12 51 = F12 52 = G12 53 = H12 54 = I12 55 = E13 56 = D13 57 = C13 58 = B13 59 = A13 60 = F13 61 = G13 |  | 62 = H13 63 = I13 64 = E14 65 = D14 66 = C14 67 = B14 68 = A14 69 = F14 70 = G14 71 = H14 72 = I14 73 = E15 74 = D15 75 = C15 76 = B15 77 = A15 78 = F15 79 = G15 80 = H15 81 = I15 82 = E16 83 = D16 84 = C16 85 = B16 86 = A16 87 = F16 88 = G16 89 = H16 90 = I16 91 = E17 92 = D17 |  | 93 = C17 94 = B17 95 = A17 96 = F17 97 = G17 98 = H17 99 = I17 100 = E6 101 = D6 102 = C6 103 = B6 104 = A6 105 = F6 106 = G6 107 = H6 108 = I6 109 = E5 110 = D5 111 = C5 112 = B5 113 = A5 114 = F5 115 = G5 116 = H5 117 = I5 118 = E4 119 = D4 120 = C4 121 = B4 122 = A4 123 = F4 |  | 124 = G4 125 = H4 126 = I4 127 = E3 128 = D3 129 = C3 130 = B3 131 = A3 132 = F3 133 = G3 134 = H3 135 = I3 136 = E2 137 = D2 138 = C2 139 = B2 140 = A2 141 = F2 142 = G2 143 = H2 144 = I2 145 = E1 146 = D1 147 = C1 148 = B1 149 = A1 150 = F1 151 = G1 152 = H1 153 = I1
> (future models?...) 0 = (none) 1 = Center
> 8 | AFPointsUsed AFPointsUsed AFPointsUsed AFPointsUsed AFPointsUsed AFPointsUsed AFPointsUsed AFPointsUsed | undef[7] undef[2] undef[5] undef[17] undef[21] undef[29] undef[20] undef[7] | (models with 51-point AF -- 5 rows: A1-9, B1-11, C1-11, D1-11, E1-9. Center point is C6) (models with 11-point AF)
> 0x0 = (none) 0x7ff = All 11 Points Bit 0 = Center Bit 1 = Top Bit 2 = Bottom Bit 3 = Mid-left Bit 4 = Upper-left |  | Bit 5 = Lower-left Bit 6 = Far Left Bit 7 = Mid-right Bit 8 = Upper-right Bit 9 = Lower-right Bit 10 = Far Right
> (models with 39-point AF -- 5 rows: A1-3, B1-11, C1-11, D1-11, E1-3. Center point is C6) (older models with 135-point AF -- 9 rows (A-I) and 15 columns (1-15). Center point is E8. The odd-numbered columns, columns 2 and 14, and the remaining corner points are not used for 41-point AF mode) (newer models with 135-point AF -- 9 rows (B-J) and 15 colums (1-15). Center point is F8) (models with 171-point AF -- 9 rows (B-J) and 19 columns (2-20). Center point is F10) (models with 153-point AF -- 9 rows (A-I) and 17 columns (1-17). Center point is E9)
> 16 | AFImageWidth | int16u | (this and the following tags are valid only for contrast-detect AF)
> 18 | AFImageHeight | int16u |
> 20 | AFAreaXPosition | int16u | (center of AF area in AFImage coordinates)
> 22 | AFAreaYPosition | int16u |
> 24 | AFAreaWidth | int16u | (size of AF area in AFImage coordinates)
> 26 | AFAreaHeight | int16u |
> 28 | ContrastDetectAFInFocus | int8u | 0 = No 1 = Yes
> 68 | PrimaryAFPoint | int8u |
> 0 = (none) 1 = E9 (Center) 2 = D9 3 = C9 4 = B9 5 = A9 6 = F9 7 = G9 8 = H9 9 = I9 10 = E10 11 = D10 12 = C10 13 = B10 14 = A10 15 = F10 16 = G10 17 = H10 18 = I10 19 = E11 20 = D11 21 = C11 22 = B11 23 = A11 24 = F11 25 = G11 26 = H11 27 = I11 28 = E8 29 = D8 30 = C8 |  | 31 = B8 32 = A8 33 = F8 34 = G8 35 = H8 36 = I8 37 = E7 38 = D7 39 = C7 40 = B7 41 = A7 42 = F7 43 = G7 44 = H7 45 = I7 46 = E12 47 = D12 48 = C12 49 = B12 50 = A12 51 = F12 52 = G12 53 = H12 54 = I12 55 = E13 56 = D13 57 = C13 58 = B13 59 = A13 60 = F13 61 = G13 |  | 62 = H13 63 = I13 64 = E14 65 = D14 66 = C14 67 = B14 68 = A14 69 = F14 70 = G14 71 = H14 72 = I14 73 = E15 74 = D15 75 = C15 76 = B15 77 = A15 78 = F15 79 = G15 80 = H15 81 = I15 82 = E16 83 = D16 84 = C16 85 = B16 86 = A16 87 = F16 88 = G16 89 = H16 90 = I16 91 = E17 92 = D17 |  | 93 = C17 94 = B17 95 = A17 96 = F17 97 = G17 98 = H17 99 = I17 100 = E6 101 = D6 102 = C6 103 = B6 104 = A6 105 = F6 106 = G6 107 = H6 108 = I6 109 = E5 110 = D5 111 = C5 112 = B5 113 = A5 114 = F5 115 = G5 116 = H5 117 = I5 118 = E4 119 = D4 120 = C4 121 = B4 122 = A4 123 = F4 |  | 124 = G4 125 = H4 126 = I4 127 = E3 128 = D3 129 = C3 130 = B3 131 = A3 132 = F3 133 = G3 134 = H3 135 = I3 136 = E2 137 = D2 138 = C2 139 = B2 140 = A2 141 = F2 142 = G2 143 = H2 144 = I2 145 = E1 146 = D1 147 = C1 148 = B1 149 = A1 150 = F1 151 = G1 152 = H1 153 = I1
> (future models?...) 0 = (none) 1 = Center
> 70 | AFImageWidth | int16u | (this and the following tags are valid only for contrast-detect AF)
> 72 | AFImageHeight | int16u |
> 74 | AFAreaXPosition | int16u | (center of AF area in AFImage coordinates)
> 76 | AFAreaYPosition | int16u |
> 78 | AFAreaWidth | int16u | (size of AF area in AFImage coordinates)
> 80 | AFAreaHeight | int16u |
> 82 | ContrastDetectAFInFocus | int8u | 0 = No 1 = Yes

## Nikon FileInfo Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FileInfoVersion | no |
> 2 | MemoryCardNumber | int16u |
> 3 | DirectoryNumber | int16u |
> 4 | FileNumber | int16u |

## Nikon AFTune Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | AFFineTune | int8u | 0 = Off 1 = On (1) 2 = On (2)
> 1 | AFFineTuneIndex | int8u | (index of saved lens)
> 2 | AFFineTuneAdj | int8s | (may only be valid for saved lenses)

## Nikon RetouchInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | RetouchInfoVersion | no |
> 5 | RetouchNEFProcessing | int8s | -1 = Off 1 = On

## Nikon BarometerInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | BarometerInfoVersion | no |
> 6 | Altitude | int32s |

## Nikon CaptureOffsets Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | IFD0_Offset | no |
> 0x0002 | PreviewIFD_Offset | no |
> 0x0003 | SubIFD_Offset | no |

## Nikon Scan Tags

This information is written by the Nikon Scan software.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0002 | FilmType | string |
> 0x0040 | MultiSample | string |
> 0x0041 | BitDepth | int16u |
> 0x0050 | MasterGain | rational64s |
> 0x0051 | ColorGain | rational64s[3] |
> 0x0060 | ScanImageEnhancer | int32u | 0 = Off 1 = On
> 0x0100 | DigitalICE | string |
> 0x0110 | ROCInfo | - | --> Nikon ROC Tags
> 0x0120 | GEMInfo | - | --> Nikon GEM Tags
> 0x0200 | DigitalDEEShadowAdj | int32u |
> 0x0201 | DigitalDEEThreshold | int32u |
> 0x0202 | DigitalDEEHighlightAdj | int32u |

## Nikon ROC Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | DigitalROC | int32u |

## Nikon GEM Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | DigitalGEM | int32u |

## Nikon CaptureOutput Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 2 | OutputImageWidth | int32u |
> 3 | OutputImageHeight | int32u |
> 4 | OutputResolution | int32u |

## Nikon Type2 Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0003 | Quality | yes |
> 0x0004 | ColorMode | yes |
> 0x0005 | ImageAdjustment | yes |
> 0x0006 | CCDSensitivity | yes |
> 0x0007 | WhiteBalance | yes |
> 0x0008 | Focus | yes |
> 0x000a | DigitalZoom | yes |
> 0x000b | Converter | yes |

## Nikon NCDT Tags

Nikon-specific QuickTime tags found in the NCDT atom of MOV videos from various Nikon models.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'NCDB' | NikonNCDB | - | --> Nikon NCDB Tags
> 'NCHD' | MakerNoteVersion | no |
> 'NCM1' | PreviewImage1 | no |
> 'NCM2' | PreviewImage2 | no |
> 'NCTG' | NikonTags | - | --> Nikon NCTG Tags
> 'NCTH' | ThumbnailImage | no |
> 'NCVW' | PreviewImage | no |

## Nikon NCDB Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Nikon NCTG Tags

These tags are found in proprietary-format records of the NCTG atom in MOV videos from some Nikon cameras.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | Make | no |
> 0x0002 | Model | no |
> 0x0003 | Software | no |
> 0x0011 | CreateDate | no |
> 0x0012 | DateTimeOriginal | no |
> 0x0013 | FrameCount | no |
> 0x0016 | FrameRate | no |
> 0x0022 | FrameWidth | no |
> 0x0023 | FrameHeight | no |
> 0x0032 | AudioChannels | no |
> 0x0033 | AudioBitsPerSample | no |
> 0x0034 | AudioSampleRate | no |
> 0x1002 | NikonDateTime | no |
> 0x1013 | ElectronicVR | no | 0 = Off 1 = On
> 0x110829a | ExposureTime | no |
> 0x110829d | FNumber | no |
> 0x1108822 | ExposureProgram | no |
> 0 = Not Defined 1 = Manual 2 = Program AE 3 = Aperture-priority AE 4 = Shutter speed priority AE 5 = Creative (Slow speed) 6 = Action (High speed) 7 = Portrait 8 = Landscape
> 0x1109204 | ExposureCompensation | no |
> 0x1109207 | MeteringMode | no |
> 0 = Unknown 1 = Average 2 = Center-weighted average 3 = Spot 4 = Multi-spot 5 = Multi-segment 6 = Partial 255 = Other
> 0x110920a | FocalLength | no |
> 0x110a434 | LensModel | no |
> 0x1200000 | GPSVersionID | no |
> 0x1200001 | GPSLatitudeRef | no | 'N' = North 'S' = South
> 0x1200002 | GPSLatitude | no |
> 0x1200003 | GPSLongitudeRef | no | 'E' = East 'W' = West
> 0x1200004 | GPSLongitude | no |
> 0x1200005 | GPSAltitudeRef | no | 0 = Above Sea Level 1 = Below Sea Level
> 0x1200006 | GPSAltitude | no |
> 0x1200007 | GPSTimeStamp | no |
> 0x1200008 | GPSSatellites | no |
> 0x1200010 | GPSImgDirectionRef | no | 'M' = Magnetic North 'T' = True North
> 0x1200011 | GPSImgDirection | no |
> 0x1200012 | GPSMapDatum | no |
> 0x120001d | GPSDateStamp | no |
> 0x2000001 | MakerNoteVersion | no |
> 0x2000005 | WhiteBalance | no |
> 0x2000007 | FocusMode | string |
> 0x200000b | WhiteBalanceFineTune | no |
> 0x200001b | CropHiSpeed | int16u[7]~ |
> 0x200001e | ColorSpace | no | 1 = sRGB 2 = Adobe RGB
> 0x200001f | VRInfo | - | --> Nikon VRInfo Tags
> 0x2000022 | ActiveD-Lighting | int16u |
> 0 = Off 1 = Low 3 = Normal 5 = High 7 = Extra High |  | 8 = Extra High 1 9 = Extra High 2 10 = Extra High 3 11 = Extra High 4 65535 = Auto
> 0x2000023 | PictureControlData | - | --> Nikon PictureControl Tags --> Nikon PictureControl2 Tags
> 0x2000024 | WorldTime | - | --> Nikon WorldTime Tags
> 0x2000025 | ISOInfo | - | --> Nikon ISOInfo Tags
> 0x200002c | UnknownInfo | - | --> Nikon UnknownInfo Tags
> 0x2000032 | UnknownInfo2 | - | --> Nikon UnknownInfo Tags
> 0x2000039 | LocationInfo | - | --> Nikon LocationInfo Tags
> 0x2000083 | LensType | no | Bit 0 = MF Bit 1 = D Bit 2 = G Bit 3 = VR
> 0x2000084 | Lens | no |
> 0x2000087 | FlashMode | int8u |
> 0 = Did Not Fire 1 = Fired, Manual 3 = Not Ready 7 = Fired, External 8 = Fired, Commander Mode 9 = Fired, TTL Mode
> 0x20000a8 | FlashInfo0100 FlashInfo0102 FlashInfo0103 FlashInfoUnknown | - - - - | --> Nikon FlashInfo0100 Tags --> Nikon FlashInfo0102 Tags --> Nikon FlashInfo0103 Tags --> Nikon FlashInfoUnknown Tags
> 0x20000ab | VariProgram | string |
> 0x20000b1 | HighISONoiseReduction | int16u |
> 0 = Off 1 = Minimal 2 = Low 3 = Medium Low |  | 4 = Normal 5 = Medium High 6 = High
> 0x20000b7 | AFInfo2 | - | --> Nikon AFInfo2 Tags

## Nikon MOV Tags

This information is found in MOV and QT videos from some Nikon cameras.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | no |
> 24 | Model | no |
> 38 | ExposureTime | no |
> 42 | FNumber | no |
> 50 | ExposureCompensation | no |
> 68 | WhiteBalance | no |
> 0 = Auto 1 = Daylight 2 = Shade |  | 3 = Fluorescent 4 = Tungsten 5 = Manual
> 72 | FocalLength | no |
> 175 | Software | no |
> 223 | ISO | no |

## Nikon AVI Tags

Nikon-specific RIFF tags found in AVI videos.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'nctg' | NikonTags | - | --> Nikon AVITags Tags
> 'ncth' | ThumbnailImage | no |
> 'ncvr' | NikonVers | - | --> Nikon AVIVers Tags
> 'ncvw' | PreviewImage | no |

## Nikon AVITags Tags

These tags and the AVIVer tags below are found in proprietary-format records of Nikon AVI videos.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0003 | Make | no |
> 0x0004 | Model | no |
> 0x0005 | Software | no |
> 0x0006 | Equipment | no |
> 0x0007 | Orientation | no |
> 1 = Horizontal (normal) 2 = Mirror horizontal 3 = Rotate 180 4 = Mirror vertical 5 = Mirror horizontal and rotate 270 CW 6 = Rotate 90 CW 7 = Mirror horizontal and rotate 90 CW 8 = Rotate 270 CW
> 0x0008 | ExposureTime | no |
> 0x0009 | FNumber | no |
> 0x000a | ExposureCompensation | no |
> 0x000b | MaxApertureValue | no |
> 0x000c | MeteringMode | no |
> 0 = Unknown 1 = Average 2 = Center-weighted average 3 = Spot 4 = Multi-spot 5 = Multi-segment 6 = Partial 255 = Other
> 0x000f | FocalLength | no |
> 0x0010 | XResolution | no |
> 0x0011 | YResolution | no |
> 0x0012 | ResolutionUnit | no | 1 = None 2 = inches 3 = cm
> 0x0013 | DateTimeOriginal | no |
> 0x0014 | CreateDate | no |
> 0x0016 | Duration | no |
> 0x0018 | FocusMode | no |
> 0x001b | DigitalZoom | no |
> 0x001d | ColorMode | no |
> 0x001e | Sharpness | no |
> 0x001f | WhiteBalance | no |
> 0x0020 | NoiseReduction | no |

## Nikon AVIVers Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | MakerNoteType | no |
> 0x0002 | MakerNoteVersion | no |

## Nikon LensID Values

The Nikon LensID is constructed as a Composite tag from the raw hex values of 8 other tags: LensIDNumber, LensFStops, MinFocalLength, MaxFocalLength, MaxApertureAtMinFocal, MaxApertureAtMaxFocal, MCUVersion and LensType, in that order. (source: http://www.rottmerhusen.com/objektives/lensid/thirdparty.html.) Multiple lenses with the same LensID are differentiated by decimal values in the list below. The user-defined "Lenses" list may be used to specify the lens for ExifTool to choose in these cases (see the sample config file for details).

> Value | LensID
> --- | ---
> '00 00 00 00 00 00 00 01' | = Manual Lens No CPU
> '00 00 00 00 00 00 E1 12' | = TC-17E II
> '00 00 00 00 00 00 F1 0C' | = TC-14E [II] or Sigma APO Tele Converter 1.4x EX DG or Kenko Teleplus PRO 300 DG 1.4x
> '00 00 00 00 00 00 F2 18' | = TC-20E [II] or Sigma APO Tele Converter 2x EX DG or Kenko Teleplus PRO 300 DG 2.0x
> '00 00 48 48 53 53 00 01' | = Loreo 40mm F11-22 3D Lens in a Cap 9005
> '00 36 1C 2D 34 3C 00 06' | = Tamron SP AF 11-18mm f/4.5-5.6 Di II LD Aspherical (IF) (A13)
> '00 3C 1F 37 30 30 00 06' | = Tokina AT-X 124 AF PRO DX (AF 12-24mm f/4)
> '00 3C 2B 44 30 30 00 06' | = Tokina AT-X 17-35 F4 PRO FX (AF 17-35mm f/4)
> '00 3C 5C 80 30 30 00 0E' | = Tokina AT-X 70-200 F4 FX VCM-S (AF 70-200mm f/4)
> '00 3E 80 A0 38 3F 00 02' | = Tamron SP AF 200-500mm f/5-6.3 Di LD (IF) (A08)
> '00 3F 2D 80 2B 40 00 06' | = Tamron AF 18-200mm f/3.5-6.3 XR Di II LD Aspherical (IF) (A14)
> '00 3F 2D 80 2C 40 00 06' | = Tamron AF 18-200mm f/3.5-6.3 XR Di II LD Aspherical (IF) Macro (A14)
> '00 3F 80 A0 38 3F 00 02' | = Tamron SP AF 200-500mm f/5-6.3 Di (A08)
> '00 40 11 11 2C 2C 00 00' | = Samyang 8mm f/3.5 Fish-Eye
> '00 40 18 2B 2C 34 00 06' | = Tokina AT-X 107 AF DX Fisheye (AF 10-17mm f/3.5-4.5)
> '00 40 2A 72 2C 3C 00 06' | = Tokina AT-X 16.5-135 DX (AF 16.5-135mm F3.5-5.6)
> '00 40 2B 2B 2C 2C 00 02' | = Tokina AT-X 17 AF PRO (AF 17mm f/3.5)
> '00 40 2D 2D 2C 2C 00 00' | = Carl Zeiss Distagon T* 3.5/18 ZF.2
> '00 40 2D 80 2C 40 00 06' | = Tamron AF 18-200mm f/3.5-6.3 XR Di II LD Aspherical (IF) Macro (A14NII)
> '00 40 2D 88 2C 40 00 06' | = Tamron AF 18-250mm f/3.5-6.3 Di II LD Aspherical (IF) Macro (A18NII)
> '00 40 2D 88 2C 40 62 06' | = Tamron AF 18-250mm f/3.5-6.3 Di II LD Aspherical (IF) Macro (A18)
> '00 40 31 31 2C 2C 00 00' | = Voigtlander Color Skopar 20mm F3.5 SLII Aspherical
> '00 40 37 80 2C 3C 00 02' | = Tokina AT-X 242 AF (AF 24-200mm f/3.5-5.6)
> '00 40 64 64 2C 2C 00 00' | = Voigtlander APO-Lanthar 90mm F3.5 SLII Close Focus
> '00 44 60 98 34 3C 00 02' | = Tokina AT-X 840 D (AF 80-400mm f/4.5-5.6)
> '00 47 10 10 24 24 00 00' | = Fisheye Nikkor 8mm f/2.8 AiS
> '00 47 25 25 24 24 00 02' | = Tamron SP AF 14mm f/2.8 Aspherical (IF) (69E)
> '00 47 3C 3C 24 24 00 00' | = Nikkor 28mm f/2.8 AiS
> '00 47 44 44 24 24 00 06' | = Tokina AT-X M35 PRO DX (AF 35mm f/2.8 Macro)
> '00 47 53 80 30 3C 00 06' | = Tamron AF 55-200mm f/4-5.6 Di II LD (A15)
> '00 48 1C 29 24 24 00 06' | = Tokina AT-X 116 PRO DX (AF 11-16mm f/2.8)
> '00 48 29 3C 24 24 00 06' | = Tokina AT-X 16-28 AF PRO FX (AF 16-28mm f/2.8)
> '00 48 29 50 24 24 00 06' | = Tokina AT-X 165 PRO DX (AF 16-50mm f/2.8)
> '00 48 32 32 24 24 00 00' | = Carl Zeiss Distagon T* 2.8/21 ZF.2
> '00 48 37 5C 24 24 00 06' | = Tokina AT-X 24-70 F2.8 PRO FX (AF 24-70mm f/2.8)
> '00 48 3C 3C 24 24 00 00' | = Voigtlander Color Skopar 28mm F2.8 SL II
> '00 48 3C 60 24 24 00 02' | = Tokina AT-X 280 AF PRO (AF 28-80mm f/2.8)
> '00 48 3C 6A 24 24 00 02' | = Tamron SP AF 28-105mm f/2.8 LD Aspherical IF (176D)
> '00 48 50 50 18 18 00 00' | = Nikkor H 50mm f/2
> '00 48 50 72 24 24 00 06' | = Tokina AT-X 535 PRO DX (AF 50-135mm f/2.8)
> '00 48 5C 80 30 30 00 0E' | = Tokina AT-X 70-200 F4 FX VCM-S (AF 70-200mm f/4)
> '00 48 5C 8E 30 3C 00 06' | = Tamron AF 70-300mm f/4-5.6 Di LD Macro 1:2 (A17NII)
> '00 48 68 68 24 24 00 00' | = Series E 100mm f/2.8
> '00 48 80 80 30 30 00 00' | = Nikkor 200mm f/4 AiS
> '00 49 30 48 22 2B 00 02' | = Tamron SP AF 20-40mm f/2.7-3.5 (166D)
> '00 4C 6A 6A 20 20 00 00' | = Nikkor 105mm f/2.5 AiS
> '00 4C 7C 7C 2C 2C 00 02' | = Tamron SP AF 180mm f/3.5 Di Model (B01)
> '00 53 2B 50 24 24 00 06' | = Tamron SP AF 17-50mm f/2.8 XR Di II LD Aspherical (IF) (A16)
> '00 54 2B 50 24 24 00 06' | = Tamron SP AF 17-50mm f/2.8 XR Di II LD Aspherical (IF) (A16NII)
> '00 54 38 38 18 18 00 00' | = Carl Zeiss Distagon T* 2/25 ZF.2
> '00 54 3C 3C 18 18 00 00' | = Carl Zeiss Distagon T* 2/28 ZF.2
> '00 54 44 44 0C 0C 00 00' | = Carl Zeiss Distagon T* 1.4/35 ZF.2
> '00 54 44 44 18 18 00 00' | = Carl Zeiss Distagon T* 2/35 ZF.2
> '00 54 48 48 18 18 00 00' | = Voigtlander Ultron 40mm F2 SLII Aspherical
> '00 54 50 50 0C 0C 00 00' | = Carl Zeiss Planar T* 1.4/50 ZF.2
> '00 54 50 50 18 18 00 00' | = Carl Zeiss Makro-Planar T* 2/50 ZF.2
> '00 54 53 53 0C 0C 00 00' | = Zeiss Otus 1.4/55
> '00 54 55 55 0C 0C 00 00' | = Voigtlander Nokton 58mm F1.4 SLII
> '00 54 56 56 30 30 00 00' | = Coastal Optical Systems 60mm 1:4 UV-VIS-IR Macro Apo
> '00 54 62 62 0C 0C 00 00' | = Carl Zeiss Planar T* 1.4/85 ZF.2
> '00 54 68 68 18 18 00 00' | = Carl Zeiss Makro-Planar T* 2/100 ZF.2
> '00 54 68 68 24 24 00 02' | = Tokina AT-X M100 AF PRO D (AF 100mm f/2.8 Macro)
> '00 54 72 72 18 18 00 00' | = Carl Zeiss Apo Sonnar T* 2/135 ZF.2
> '00 54 8E 8E 24 24 00 02' | = Tokina AT-X 300 AF PRO (AF 300mm f/2.8)
> '00 57 50 50 14 14 00 00' | = Nikkor 50mm f/1.8 AI
> '00 58 64 64 20 20 00 00' | = Soligor C/D Macro MC 90mm f/2.5
> '01 00 00 00 00 00 02 00' | = TC-16A
> '01 00 00 00 00 00 08 00' | = TC-16A
> '01 54 62 62 0C 0C 00 00' | = Zeiss Otus 1.4/85
> '01 58 50 50 14 14 02 00' | = AF Nikkor 50mm f/1.8
> '01 58 50 50 14 14 05 00' | = AF Nikkor 50mm f/1.8
> '02 2F 98 98 3D 3D 02 00' | = Sigma APO 400mm F5.6
> '02 34 A0 A0 44 44 02 00' | = Sigma APO 500mm F7.2
> '02 37 5E 8E 35 3D 02 00' | = Sigma 75-300mm F4.5-5.6 APO
> '02 37 A0 A0 34 34 02 00' | = Sigma APO 500mm F4.5
> '02 3A 37 50 31 3D 02 00' | = Sigma 24-50mm F4-5.6 UC
> '02 3A 5E 8E 32 3D 02 00' | = Sigma 75-300mm F4.0-5.6
> '02 3B 44 61 30 3D 02 00' | = Sigma 35-80mm F4-5.6
> '02 3C B0 B0 3C 3C 02 00' | = Sigma APO 800mm F5.6
> '02 3F 24 24 2C 2C 02 00' | = Sigma 14mm F3.5
> '02 3F 3C 5C 2D 35 02 00' | = Sigma 28-70mm F3.5-4.5 UC
> '02 40 44 5C 2C 34 02 00' | = Exakta AF 35-70mm 1:3.5-4.5 MC
> '02 40 44 73 2B 36 02 00' | = Sigma 35-135mm F3.5-4.5 a
> '02 40 5C 82 2C 35 02 00' | = Sigma APO 70-210mm F3.5-4.5
> '02 42 44 5C 2A 34 02 00' | = AF Zoom-Nikkor 35-70mm f/3.3-4.5
> '02 42 44 5C 2A 34 08 00' | = AF Zoom-Nikkor 35-70mm f/3.3-4.5
> '02 46 37 37 25 25 02 00' | = Sigma 24mm F2.8 Super Wide II Macro
> '02 46 3C 5C 25 25 02 00' | = Sigma 28-70mm F2.8
> '02 46 5C 82 25 25 02 00' | = Sigma 70-210mm F2.8 APO
> '02 48 50 50 24 24 02 00' | = Sigma Macro 50mm F2.8
> '02 48 65 65 24 24 02 00' | = Sigma Macro 90mm F2.8
> '03 43 5C 81 35 35 02 00' | = Soligor AF C/D Zoom UMCS 70-210mm 1:4.5
> '03 48 5C 81 30 30 02 00' | = AF Zoom-Nikkor 70-210mm f/4
> '04 48 3C 3C 24 24 03 00' | = AF Nikkor 28mm f/2.8
> '05 54 50 50 0C 0C 04 00' | = AF Nikkor 50mm f/1.4
> '06 3F 68 68 2C 2C 06 00' | = Cosina AF 100mm F3.5 Macro
> '06 54 53 53 24 24 06 00' | = AF Micro-Nikkor 55mm f/2.8
> '07 36 3D 5F 2C 3C 03 00' | = Cosina AF Zoom 28-80mm F3.5-5.6 MC Macro
> '07 3E 30 43 2D 35 03 00' | = Soligor AF Zoom 19-35mm 1:3.5-4.5 MC
> '07 40 2F 44 2C 34 03 02' | = Tamron AF 19-35mm f/3.5-4.5 (A10)
> '07 40 30 45 2D 35 03 02' | = Tamron AF 19-35mm f/3.5-4.5 (A10)
> '07 40 3C 5C 2C 35 03 00' | = Tokina AF 270 II (AF 28-70mm f/3.5-4.5)
> '07 40 3C 62 2C 34 03 00' | = AF Zoom-Nikkor 28-85mm f/3.5-4.5
> '07 46 2B 44 24 30 03 02' | = Tamron SP AF 17-35mm f/2.8-4 Di LD Aspherical (IF) (A05)
> '07 46 3D 6A 25 2F 03 00' | = Cosina AF Zoom 28-105mm F2.8-3.8 MC
> '07 47 3C 5C 25 35 03 00' | = Tokina AF 287 SD (AF 28-70mm f/2.8-4.5)
> '07 48 3C 5C 24 24 03 00' | = Tokina AT-X 287 AF (AF 28-70mm f/2.8)
> '08 40 44 6A 2C 34 04 00' | = AF Zoom-Nikkor 35-105mm f/3.5-4.5
> '09 48 37 37 24 24 04 00' | = AF Nikkor 24mm f/2.8
> '0A 48 8E 8E 24 24 03 00' | = AF Nikkor 300mm f/2.8 IF-ED
> '0A 48 8E 8E 24 24 05 00' | = AF Nikkor 300mm f/2.8 IF-ED N
> '0B 3E 3D 7F 2F 3D 0E 00' | = Tamron AF 28-200mm f/3.8-5.6 (71D)
> '0B 3E 3D 7F 2F 3D 0E 02' | = Tamron AF 28-200mm f/3.8-5.6D (171D)
> '0B 48 7C 7C 24 24 05 00' | = AF Nikkor 180mm f/2.8 IF-ED
> '0D 40 44 72 2C 34 07 00' | = AF Zoom-Nikkor 35-135mm f/3.5-4.5
> '0E 48 5C 81 30 30 05 00' | = AF Zoom-Nikkor 70-210mm f/4
> '0E 4A 31 48 23 2D 0E 02' | = Tamron SP AF 20-40mm f/2.7-3.5 (166D)
> '0F 58 50 50 14 14 05 00' | = AF Nikkor 50mm f/1.8 N
> '10 3D 3C 60 2C 3C D2 02' | = Tamron AF 28-80mm f/3.5-5.6 Aspherical (177D)
> '10 48 8E 8E 30 30 08 00' | = AF Nikkor 300mm f/4 IF-ED
> '11 48 44 5C 24 24 08 00' | = AF Zoom-Nikkor 35-70mm f/2.8
> '11 48 44 5C 24 24 15 00' | = AF Zoom-Nikkor 35-70mm f/2.8
> '12 36 5C 81 35 3D 09 00' | = Cosina AF Zoom 70-210mm F4.5-5.6 MC Macro
> '12 36 69 97 35 42 09 00' | = Soligor AF Zoom 100-400mm 1:4.5-6.7 MC
> '12 38 69 97 35 42 09 02' | = Promaster Spectrum 7 100-400mm F4.5-6.7
> '12 39 5C 8E 34 3D 08 02' | = Cosina AF Zoom 70-300mm F4.5-5.6 MC Macro
> '12 3B 68 8D 3D 43 09 02' | = Cosina AF Zoom 100-300mm F5.6-6.7 MC Macro
> '12 3B 98 98 3D 3D 09 00' | = Tokina AT-X 400 AF SD (AF 400mm f/5.6)
> '12 3D 3C 80 2E 3C DF 02' | = Tamron AF 28-200mm f/3.8-5.6 AF Aspherical LD (IF) (271D)
> '12 44 5E 8E 34 3C 09 00' | = Tokina AF 730 (AF 75-300mm F4.5-5.6)
> '12 48 5C 81 30 3C 09 00' | = AF Nikkor 70-210mm f/4-5.6
> '12 4A 5C 81 31 3D 09 00' | = Soligor AF C/D Auto Zoom+Macro 70-210mm 1:4-5.6 UMCS
> '13 42 37 50 2A 34 0B 00' | = AF Zoom-Nikkor 24-50mm f/3.3-4.5
> '14 48 60 80 24 24 0B 00' | = AF Zoom-Nikkor 80-200mm f/2.8 ED
> '14 48 68 8E 30 30 0B 00' | = Tokina AT-X 340 AF (AF 100-300mm f/4)
> '14 54 60 80 24 24 0B 00' | = Tokina AT-X 828 AF (AF 80-200mm f/2.8)
> '15 4C 62 62 14 14 0C 00' | = AF Nikkor 85mm f/1.8
> '17 3C A0 A0 30 30 0F 00' | = Nikkor 500mm f/4 P ED IF
> '17 3C A0 A0 30 30 11 00' | = Nikkor 500mm f/4 P ED IF
> '18 40 44 72 2C 34 0E 00' | = AF Zoom-Nikkor 35-135mm f/3.5-4.5 N
> '1A 54 44 44 18 18 11 00' | = AF Nikkor 35mm f/2
> '1B 44 5E 8E 34 3C 10 00' | = AF Zoom-Nikkor 75-300mm f/4.5-5.6
> '1C 48 30 30 24 24 12 00' | = AF Nikkor 20mm f/2.8
> '1D 42 44 5C 2A 34 12 00' | = AF Zoom-Nikkor 35-70mm f/3.3-4.5 N
> '1E 54 56 56 24 24 13 00' | = AF Micro-Nikkor 60mm f/2.8
> '1E 5D 64 64 20 20 13 00' | = Tamron SP AF 90mm f/2.5 (52E)
> '1F 54 6A 6A 24 24 14 00' | = AF Micro-Nikkor 105mm f/2.8
> '20 3C 80 98 3D 3D 1E 02' | = Tamron AF 200-400mm f/5.6 LD IF (75D)
> '20 48 60 80 24 24 15 00' | = AF Zoom-Nikkor 80-200mm f/2.8 ED
> '20 5A 64 64 20 20 14 00' | = Tamron SP AF 90mm f/2.5 Macro (152E)
> '21 40 3C 5C 2C 34 16 00' | = AF Zoom-Nikkor 28-70mm f/3.5-4.5
> '21 56 8E 8E 24 24 14 00' | = Tamron SP AF 300mm f/2.8 LD-IF (60E)
> '22 48 72 72 18 18 16 00' | = AF DC-Nikkor 135mm f/2
> '22 53 64 64 24 24 E0 02' | = Tamron SP AF 90mm f/2.8 Macro 1:1 (72E)
> '23 30 BE CA 3C 48 17 00' | = Zoom-Nikkor 1200-1700mm f/5.6-8 P ED IF
> '24 44 60 98 34 3C 1A 02' | = Tokina AT-X 840 AF-II (AF 80-400mm f/4.5-5.6)
> '24 48 60 80 24 24 1A 02' | = AF Zoom-Nikkor 80-200mm f/2.8D ED
> '24 54 60 80 24 24 1A 02' | = Tokina AT-X 828 AF PRO (AF 80-200mm f/2.8)
> '25 44 44 8E 34 42 1B 02' | = Tokina AF 353 (AF 35-300mm f/4.5-6.7)
> '25 48 3C 5C 24 24 1B 02.1' | = Tokina AT-X 270 AF PRO II (AF 28-70mm f/2.6-2.8)
> '25 48 3C 5C 24 24 1B 02.2' | = Tokina AT-X 287 AF PRO SV (AF 28-70mm f/2.8)
> '25 48 44 5C 24 24 1B 02' | = AF Zoom-Nikkor 35-70mm f/2.8D
> '25 48 44 5C 24 24 3A 02' | = AF Zoom-Nikkor 35-70mm f/2.8D
> '25 48 44 5C 24 24 52 02' | = AF Zoom-Nikkor 35-70mm f/2.8D
> '26 3C 54 80 30 3C 1C 06' | = Sigma 55-200mm F4-5.6 DC
> '26 3C 5C 82 30 3C 1C 02' | = Sigma 70-210mm F4-5.6 UC-II
> '26 3C 5C 8E 30 3C 1C 02' | = Sigma 70-300mm F4-5.6 DG Macro
> '26 3C 98 98 3C 3C 1C 02' | = Sigma APO Tele Macro 400mm F5.6
> '26 3D 3C 80 2F 3D 1C 02' | = Sigma 28-300mm F3.8-5.6 Aspherical
> '26 3E 3C 6A 2E 3C 1C 02' | = Sigma 28-105mm F3.8-5.6 UC-III Aspherical IF
> '26 40 27 3F 2C 34 1C 02' | = Sigma 15-30mm F3.5-4.5 EX DG Aspherical DF
> '26 40 2D 44 2B 34 1C 02' | = Sigma 18-35mm F3.5-4.5 Aspherical
> '26 40 2D 50 2C 3C 1C 06' | = Sigma 18-50mm F3.5-5.6 DC
> '26 40 2D 70 2B 3C 1C 06' | = Sigma 18-125mm F3.5-5.6 DC
> '26 40 2D 80 2C 40 1C 06' | = Sigma 18-200mm F3.5-6.3 DC
> '26 40 37 5C 2C 3C 1C 02' | = Sigma 24-70mm F3.5-5.6 Aspherical HF
> '26 40 3C 5C 2C 34 1C 02' | = AF Zoom-Nikkor 28-70mm f/3.5-4.5D
> '26 40 3C 60 2C 3C 1C 02' | = Sigma 28-80mm F3.5-5.6 Mini Zoom Macro II Aspherical
> '26 40 3C 65 2C 3C 1C 02' | = Sigma 28-90mm F3.5-5.6 Macro
> '26 40 3C 80 2B 3C 1C 02' | = Sigma 28-200mm F3.5-5.6 Compact Aspherical Hyperzoom Macro
> '26 40 3C 80 2C 3C 1C 02' | = Sigma 28-200mm F3.5-5.6 Compact Aspherical Hyperzoom Macro
> '26 40 3C 8E 2C 40 1C 02' | = Sigma 28-300mm F3.5-6.3 Macro
> '26 40 7B A0 34 40 1C 02' | = Sigma APO 170-500mm F5-6.3 Aspherical RF
> '26 41 3C 8E 2C 40 1C 02' | = Sigma 28-300mm F3.5-6.3 DG Macro
> '26 44 73 98 34 3C 1C 02' | = Sigma 135-400mm F4.5-5.6 APO Aspherical
> '26 48 11 11 30 30 1C 02' | = Sigma 8mm F4 EX Circular Fisheye
> '26 48 27 27 24 24 1C 02' | = Sigma 15mm F2.8 EX Diagonal Fisheye
> '26 48 2D 50 24 24 1C 06' | = Sigma 18-50mm F2.8 EX DC
> '26 48 31 49 24 24 1C 02' | = Sigma 20-40mm F2.8
> '26 48 37 56 24 24 1C 02' | = Sigma 24-60mm F2.8 EX DG
> '26 48 3C 5C 24 24 1C 06' | = Sigma 28-70mm F2.8 EX DG
> '26 48 3C 5C 24 30 1C 02' | = Sigma 28-70mm F2.8-4 DG
> '26 48 3C 6A 24 30 1C 02' | = Sigma 28-105mm F2.8-4 Aspherical
> '26 48 8E 8E 30 30 1C 02' | = Sigma APO Tele Macro 300mm F4
> '26 54 2B 44 24 30 1C 02' | = Sigma 17-35mm F2.8-4 EX Aspherical
> '26 54 37 5C 24 24 1C 02' | = Sigma 24-70mm F2.8 EX DG Macro
> '26 54 37 73 24 34 1C 02' | = Sigma 24-135mm F2.8-4.5
> '26 54 3C 5C 24 24 1C 02' | = Sigma 28-70mm F2.8 EX
> '26 58 31 31 14 14 1C 02' | = Sigma 20mm F1.8 EX DG Aspherical RF
> '26 58 37 37 14 14 1C 02' | = Sigma 24mm F1.8 EX DG Aspherical Macro
> '26 58 3C 3C 14 14 1C 02' | = Sigma 28mm F1.8 EX DG Aspherical Macro
> '27 48 8E 8E 24 24 1D 02' | = AF-I Nikkor 300mm f/2.8D IF-ED
> '27 48 8E 8E 24 24 E1 02' | = AF-I Nikkor 300mm f/2.8D IF-ED + TC-17E
> '27 48 8E 8E 24 24 F1 02' | = AF-I Nikkor 300mm f/2.8D IF-ED + TC-14E
> '27 48 8E 8E 24 24 F2 02' | = AF-I Nikkor 300mm f/2.8D IF-ED + TC-20E
> '27 48 8E 8E 30 30 1D 02' | = Tokina AT-X 304 AF (AF 300mm f/4.0)
> '27 54 8E 8E 24 24 1D 02' | = Tamron SP AF 300mm f/2.8 LD-IF (360E)
> '28 3C A6 A6 30 30 1D 02' | = AF-I Nikkor 600mm f/4D IF-ED
> '28 3C A6 A6 30 30 E1 02' | = AF-I Nikkor 600mm f/4D IF-ED + TC-17E
> '28 3C A6 A6 30 30 F1 02' | = AF-I Nikkor 600mm f/4D IF-ED + TC-14E
> '28 3C A6 A6 30 30 F2 02' | = AF-I Nikkor 600mm f/4D IF-ED + TC-20E
> '2A 54 3C 3C 0C 0C 26 02' | = AF Nikkor 28mm f/1.4D
> '2B 3C 44 60 30 3C 1F 02' | = AF Zoom-Nikkor 35-80mm f/4-5.6D
> '2C 48 6A 6A 18 18 27 02' | = AF DC-Nikkor 105mm f/2D
> '2D 48 80 80 30 30 21 02' | = AF Micro-Nikkor 200mm f/4D IF-ED
> '2E 48 5C 82 30 3C 22 02' | = AF Nikkor 70-210mm f/4-5.6D
> '2E 48 5C 82 30 3C 28 02' | = AF Nikkor 70-210mm f/4-5.6D
> '2F 40 30 44 2C 34 29 02.1' | = Tokina AF 235 II (AF 20-35mm f/3.5-4.5)
> '2F 40 30 44 2C 34 29 02.2' | = Tokina AF 193 (AF 19-35mm f/3.5-4.5)
> '2F 48 30 44 24 24 29 02.1' | = AF Zoom-Nikkor 20-35mm f/2.8D IF
> '2F 48 30 44 24 24 29 02.2' | = Tokina AT-X 235 AF PRO (AF 20-35mm f/2.8)
> '30 48 98 98 24 24 24 02' | = AF-I Nikkor 400mm f/2.8D IF-ED
> '30 48 98 98 24 24 E1 02' | = AF-I Nikkor 400mm f/2.8D IF-ED + TC-17E
> '30 48 98 98 24 24 F1 02' | = AF-I Nikkor 400mm f/2.8D IF-ED + TC-14E
> '30 48 98 98 24 24 F2 02' | = AF-I Nikkor 400mm f/2.8D IF-ED + TC-20E
> '31 54 56 56 24 24 25 02' | = AF Micro-Nikkor 60mm f/2.8D
> '32 53 64 64 24 24 35 02' | = Tamron SP AF 90mm f/2.8 [Di] Macro 1:1 (172E/272E)
> '32 54 50 50 24 24 35 02' | = Sigma Macro 50mm F2.8 EX DG
> '32 54 6A 6A 24 24 35 02.1' | = AF Micro-Nikkor 105mm f/2.8D
> '32 54 6A 6A 24 24 35 02.2' | = Sigma Macro 105mm F2.8 EX DG
> '33 48 2D 2D 24 24 31 02' | = AF Nikkor 18mm f/2.8D
> '33 54 3C 5E 24 24 62 02' | = Tamron SP AF 28-75mm f/2.8 XR Di LD Aspherical (IF) Macro (A09)
> '34 48 29 29 24 24 32 02' | = AF Fisheye Nikkor 16mm f/2.8D
> '35 3C A0 A0 30 30 33 02' | = AF-I Nikkor 500mm f/4D IF-ED
> '35 3C A0 A0 30 30 E1 02' | = AF-I Nikkor 500mm f/4D IF-ED + TC-17E
> '35 3C A0 A0 30 30 F1 02' | = AF-I Nikkor 500mm f/4D IF-ED + TC-14E
> '35 3C A0 A0 30 30 F2 02' | = AF-I Nikkor 500mm f/4D IF-ED + TC-20E
> '36 48 37 37 24 24 34 02' | = AF Nikkor 24mm f/2.8D
> '37 48 30 30 24 24 36 02' | = AF Nikkor 20mm f/2.8D
> '38 4C 62 62 14 14 37 02' | = AF Nikkor 85mm f/1.8D
> '3A 40 3C 5C 2C 34 39 02' | = AF Zoom-Nikkor 28-70mm f/3.5-4.5D
> '3B 48 44 5C 24 24 3A 02' | = AF Zoom-Nikkor 35-70mm f/2.8D N
> '3C 48 60 80 24 24 3B 02' | = AF Zoom-Nikkor 80-200mm f/2.8D ED
> '3D 3C 44 60 30 3C 3E 02' | = AF Zoom-Nikkor 35-80mm f/4-5.6D
> '3E 48 3C 3C 24 24 3D 02' | = AF Nikkor 28mm f/2.8D
> '3F 40 44 6A 2C 34 45 02' | = AF Zoom-Nikkor 35-105mm f/3.5-4.5D
> '41 48 7C 7C 24 24 43 02' | = AF Nikkor 180mm f/2.8D IF-ED
> '42 54 44 44 18 18 44 02' | = AF Nikkor 35mm f/2D
> '43 54 50 50 0C 0C 46 02' | = AF Nikkor 50mm f/1.4D
> '44 44 60 80 34 3C 47 02' | = AF Zoom-Nikkor 80-200mm f/4.5-5.6D
> '45 3D 3C 60 2C 3C 48 02' | = Tamron AF 28-80mm f/3.5-5.6 Aspherical (177D)
> '45 40 3C 60 2C 3C 48 02' | = AF Zoom-Nikkor 28-80mm f/3.5-5.6D
> '45 41 37 72 2C 3C 48 02' | = Tamron SP AF 24-135mm f/3.5-5.6 AD Aspherical (IF) Macro (190D)
> '46 3C 44 60 30 3C 49 02' | = AF Zoom-Nikkor 35-80mm f/4-5.6D N
> '47 42 37 50 2A 34 4A 02' | = AF Zoom-Nikkor 24-50mm f/3.3-4.5D
> '48 38 1F 37 34 3C 4B 06' | = Sigma 12-24mm F4.5-5.6 EX DG Aspherical HSM
> '48 3C 19 31 30 3C 4B 06' | = Sigma 10-20mm F4-5.6 EX DC HSM
> '48 3C 50 A0 30 40 4B 02' | = Sigma 50-500mm F4-6.3 EX APO RF HSM
> '48 3C 8E B0 3C 3C 4B 02' | = Sigma APO 300-800mm F5.6 EX DG HSM
> '48 3C B0 B0 3C 3C 4B 02' | = Sigma APO 800mm F5.6 EX HSM
> '48 44 A0 A0 34 34 4B 02' | = Sigma APO 500mm F4.5 EX HSM
> '48 48 24 24 24 24 4B 02' | = Sigma 14mm F2.8 EX Aspherical HSM
> '48 48 2B 44 24 30 4B 06' | = Sigma 17-35mm F2.8-4 EX DG Aspherical HSM
> '48 48 68 8E 30 30 4B 02' | = Sigma APO 100-300mm F4 EX IF HSM
> '48 48 76 76 24 24 4B 06' | = Sigma APO Macro 150mm F2.8 EX DG HSM
> '48 48 8E 8E 24 24 4B 02' | = AF-S Nikkor 300mm f/2.8D IF-ED
> '48 48 8E 8E 24 24 E1 02' | = AF-S Nikkor 300mm f/2.8D IF-ED + TC-17E
> '48 48 8E 8E 24 24 F1 02' | = AF-S Nikkor 300mm f/2.8D IF-ED + TC-14E
> '48 48 8E 8E 24 24 F2 02' | = AF-S Nikkor 300mm f/2.8D IF-ED + TC-20E
> '48 4C 7C 7C 2C 2C 4B 02' | = Sigma APO Macro 180mm F3.5 EX DG HSM
> '48 4C 7D 7D 2C 2C 4B 02' | = Sigma APO Macro 180mm F3.5 EX DG HSM
> '48 54 3E 3E 0C 0C 4B 06' | = Sigma 30mm F1.4 EX DC HSM
> '48 54 5C 80 24 24 4B 02' | = Sigma 70-200mm F2.8 EX APO IF HSM
> '48 54 6F 8E 24 24 4B 02' | = Sigma APO 120-300mm F2.8 EX DG HSM
> '48 54 8E 8E 24 24 4B 02' | = Sigma APO 300mm F2.8 EX DG HSM
> '49 3C A6 A6 30 30 4C 02' | = AF-S Nikkor 600mm f/4D IF-ED
> '49 3C A6 A6 30 30 E1 02' | = AF-S Nikkor 600mm f/4D IF-ED + TC-17E
> '49 3C A6 A6 30 30 F1 02' | = AF-S Nikkor 600mm f/4D IF-ED + TC-14E
> '49 3C A6 A6 30 30 F2 02' | = AF-S Nikkor 600mm f/4D IF-ED + TC-20E
> '4A 40 11 11 2C 0C 4D 02' | = Samyang 8mm f/3.5 Fish-Eye CS
> '4A 48 1E 1E 24 0C 4D 02' | = Samyang 12mm f/2.8 ED AS NCS Fish-Eye
> '4A 48 24 24 24 0C 4D 02' | = Samyang AE 14mm f/2.8 ED AS IF UMC
> '4A 54 29 29 18 0C 4D 02' | = Samyang 16mm f/2.0 ED AS UMC CS
> '4A 54 62 62 0C 0C 4D 02' | = AF Nikkor 85mm f/1.4D IF
> '4A 60 36 36 0C 0C 4D 02' | = Samyang 24mm f/1.4 ED AS UMC
> '4A 60 44 44 0C 0C 4D 02' | = Samyang 35mm f/1.4 AS UMC
> '4A 60 62 62 0C 0C 4D 02' | = Samyang AE 85mm f/1.4 AS IF UMC
> '4B 3C A0 A0 30 30 4E 02' | = AF-S Nikkor 500mm f/4D IF-ED
> '4B 3C A0 A0 30 30 E1 02' | = AF-S Nikkor 500mm f/4D IF-ED + TC-17E
> '4B 3C A0 A0 30 30 F1 02' | = AF-S Nikkor 500mm f/4D IF-ED + TC-14E
> '4B 3C A0 A0 30 30 F2 02' | = AF-S Nikkor 500mm f/4D IF-ED + TC-20E
> '4C 40 37 6E 2C 3C 4F 02' | = AF Zoom-Nikkor 24-120mm f/3.5-5.6D IF
> '4D 3E 3C 80 2E 3C 62 02' | = Tamron AF 28-200mm f/3.8-5.6 XR Aspherical (IF) Macro (A03N)
> '4D 40 3C 80 2C 3C 62 02' | = AF Zoom-Nikkor 28-200mm f/3.5-5.6D IF
> '4D 41 3C 8E 2B 40 62 02' | = Tamron AF 28-300mm f/3.5-6.3 XR Di LD Aspherical (IF) (A061)
> '4D 41 3C 8E 2C 40 62 02' | = Tamron AF 28-300mm f/3.5-6.3 XR LD Aspherical (IF) (185D)
> '4E 48 72 72 18 18 51 02' | = AF DC-Nikkor 135mm f/2D
> '4F 40 37 5C 2C 3C 53 06' | = IX-Nikkor 24-70mm f/3.5-5.6
> '50 48 56 7C 30 3C 54 06' | = IX-Nikkor 60-180mm f/4-5.6
> '52 54 44 44 18 18 00 00' | = Zeiss Milvus 35mm f/2
> '53 48 60 80 24 24 57 02' | = AF Zoom-Nikkor 80-200mm f/2.8D ED
> '53 48 60 80 24 24 60 02' | = AF Zoom-Nikkor 80-200mm f/2.8D ED
> '53 54 50 50 0C 0C 00 00' | = Zeiss Milvus 50mm f/1.4
> '54 44 5C 7C 34 3C 58 02' | = AF Zoom-Micro Nikkor 70-180mm f/4.5-5.6D ED
> '54 44 5C 7C 34 3C 61 02' | = AF Zoom-Micro Nikkor 70-180mm f/4.5-5.6D ED
> '54 54 50 50 18 18 00 00' | = Zeiss Milvus 50mm f/2 Macro
> '55 54 62 62 0C 0C 00 00' | = Zeiss Milvus 85mm f/1.4
> '56 3C 5C 8E 30 3C 1C 02' | = Sigma 70-300mm F4-5.6 APO Macro Super II
> '56 48 5C 8E 30 3C 5A 02' | = AF Zoom-Nikkor 70-300mm f/4-5.6D ED
> '56 54 68 68 18 18 00 00' | = Zeiss Milvus 100mm f/2 Macro
> '59 48 98 98 24 24 5D 02' | = AF-S Nikkor 400mm f/2.8D IF-ED
> '59 48 98 98 24 24 E1 02' | = AF-S Nikkor 400mm f/2.8D IF-ED + TC-17E
> '59 48 98 98 24 24 F1 02' | = AF-S Nikkor 400mm f/2.8D IF-ED + TC-14E
> '59 48 98 98 24 24 F2 02' | = AF-S Nikkor 400mm f/2.8D IF-ED + TC-20E
> '5A 3C 3E 56 30 3C 5E 06' | = IX-Nikkor 30-60mm f/4-5.6
> '5B 44 56 7C 34 3C 5F 06' | = IX-Nikkor 60-180mm f/4.5-5.6
> '5D 48 3C 5C 24 24 63 02' | = AF-S Zoom-Nikkor 28-70mm f/2.8D IF-ED
> '5E 48 60 80 24 24 64 02' | = AF-S Zoom-Nikkor 80-200mm f/2.8D IF-ED
> '5F 40 3C 6A 2C 34 65 02' | = AF Zoom-Nikkor 28-105mm f/3.5-4.5D IF
> '60 40 3C 60 2C 3C 66 02' | = AF Zoom-Nikkor 28-80mm f/3.5-5.6D
> '61 44 5E 86 34 3C 67 02' | = AF Zoom-Nikkor 75-240mm f/4.5-5.6D
> '63 48 2B 44 24 24 68 02' | = AF-S Nikkor 17-35mm f/2.8D IF-ED
> '64 00 62 62 24 24 6A 02' | = PC Micro-Nikkor 85mm f/2.8D
> '65 44 60 98 34 3C 6B 0A' | = AF VR Zoom-Nikkor 80-400mm f/4.5-5.6D ED
> '66 40 2D 44 2C 34 6C 02' | = AF Zoom-Nikkor 18-35mm f/3.5-4.5D IF-ED
> '67 48 37 62 24 30 6D 02' | = AF Zoom-Nikkor 24-85mm f/2.8-4D IF
> '67 54 37 5C 24 24 1C 02' | = Sigma 24-70mm F2.8 EX DG Macro
> '68 42 3C 60 2A 3C 6E 06' | = AF Zoom-Nikkor 28-80mm f/3.3-5.6G
> '69 47 5C 8E 30 3C 00 02' | = Tamron AF 70-300mm f/4-5.6 Di LD Macro 1:2 (A17N)
> '69 48 5C 8E 30 3C 6F 02' | = Tamron AF 70-300mm f/4-5.6 LD Macro 1:2 (572D/772D)
> '69 48 5C 8E 30 3C 6F 06' | = AF Zoom-Nikkor 70-300mm f/4-5.6G
> '6A 48 8E 8E 30 30 70 02' | = AF-S Nikkor 300mm f/4D IF-ED
> '6B 48 24 24 24 24 71 02' | = AF Nikkor ED 14mm f/2.8D
> '6D 48 8E 8E 24 24 73 02' | = AF-S Nikkor 300mm f/2.8D IF-ED II
> '6E 48 98 98 24 24 74 02' | = AF-S Nikkor 400mm f/2.8D IF-ED II
> '6F 3C A0 A0 30 30 75 02' | = AF-S Nikkor 500mm f/4D IF-ED II
> '70 3C A6 A6 30 30 76 02' | = AF-S Nikkor 600mm f/4D IF-ED II
> '72 48 4C 4C 24 24 77 00' | = Nikkor 45mm f/2.8 P
> '74 40 37 62 2C 34 78 06' | = AF-S Zoom-Nikkor 24-85mm f/3.5-4.5G IF-ED
> '75 40 3C 68 2C 3C 79 06' | = AF Zoom-Nikkor 28-100mm f/3.5-5.6G
> '76 58 50 50 14 14 7A 02' | = AF Nikkor 50mm f/1.8D
> '77 44 60 98 34 3C 7B 0E' | = Sigma 80-400mm f4.5-5.6 APO DG D OS
> '77 44 61 98 34 3C 7B 0E' | = Sigma 80-400mm F4.5-5.6 EX OS
> '77 48 5C 80 24 24 7B 0E' | = AF-S VR Zoom-Nikkor 70-200mm f/2.8G IF-ED
> '78 40 37 6E 2C 3C 7C 0E' | = AF-S VR Zoom-Nikkor 24-120mm f/3.5-5.6G IF-ED
> '79 40 11 11 2C 2C 1C 06' | = Sigma 8mm F3.5 EX Circular Fisheye
> '79 40 3C 80 2C 3C 7F 06' | = AF Zoom-Nikkor 28-200mm f/3.5-5.6G IF-ED
> '79 48 3C 5C 24 24 1C 06' | = Sigma 28-70mm F2.8 EX DG
> '79 48 5C 5C 24 24 1C 06' | = Sigma Macro 70mm F2.8 EX DG
> '79 54 31 31 0C 0C 4B 06' | = Sigma 20mm F1.4 DG HSM | A
> '7A 3B 53 80 30 3C 4B 06' | = Sigma 55-200mm F4-5.6 DC HSM
> '7A 3C 1F 37 30 30 7E 06.1' | = AF-S DX Zoom-Nikkor 12-24mm f/4G IF-ED
> '7A 3C 1F 37 30 30 7E 06.2' | = Tokina AT-X 124 AF PRO DX II (AF 12-24mm f/4)
> '7A 3C 1F 3C 30 30 7E 06' | = Tokina AT-X 12-28 PRO DX (AF 12-28mm f/4)
> '7A 40 2D 50 2C 3C 4B 06' | = Sigma 18-50mm F3.5-5.6 DC HSM
> '7A 40 2D 80 2C 40 4B 0E' | = Sigma 18-200mm F3.5-6.3 DC OS HSM
> '7A 47 2B 5C 24 34 4B 06' | = Sigma 17-70mm F2.8-4.5 DC Macro Asp. IF HSM
> '7A 47 50 76 24 24 4B 06' | = Sigma 50-150mm F2.8 EX APO DC HSM
> '7A 48 1C 29 24 24 7E 06' | = Tokina AT-X 116 PRO DX II (AF 11-16mm f/2.8)
> '7A 48 1C 30 24 24 7E 06' | = Tokina AT-X 11-20 F2.8 PRO DX (AF 11-20mm f/2.8)
> '7A 48 2B 5C 24 34 4B 06' | = Sigma 17-70mm F2.8-4.5 DC Macro Asp. IF HSM
> '7A 48 2D 50 24 24 4B 06' | = Sigma 18-50mm F2.8 EX DC Macro
> '7A 48 5C 80 24 24 4B 06' | = Sigma 70-200mm F2.8 EX APO DG Macro HSM II
> '7A 54 6E 8E 24 24 4B 02' | = Sigma APO 120-300mm F2.8 EX DG HSM
> '7B 48 80 98 30 30 80 0E' | = AF-S VR Zoom-Nikkor 200-400mm f/4G IF-ED
> '7D 48 2B 53 24 24 82 06' | = AF-S DX Zoom-Nikkor 17-55mm f/2.8G IF-ED
> '7F 40 2D 5C 2C 34 84 06' | = AF-S DX Zoom-Nikkor 18-70mm f/3.5-4.5G IF-ED
> '7F 48 2B 5C 24 34 1C 06' | = Sigma 17-70mm F2.8-4.5 DC Macro Asp. IF
> '7F 48 2D 50 24 24 1C 06' | = Sigma 18-50mm F2.8 EX DC Macro
> '80 48 1A 1A 24 24 85 06' | = AF DX Fisheye-Nikkor 10.5mm f/2.8G ED
> '81 34 76 A6 38 40 4B 0E' | = Sigma 150-600mm F5-6.3 DG OS HSM | S
> '81 54 80 80 18 18 86 0E' | = AF-S VR Nikkor 200mm f/2G IF-ED
> '82 34 76 A6 38 40 4B 0E' | = Sigma 150-600mm F5-6.3 DG OS HSM | C
> '82 48 8E 8E 24 24 87 0E' | = AF-S VR Nikkor 300mm f/2.8G IF-ED
> '83 00 B0 B0 5A 5A 88 04' | = FSA-L2, EDG 65, 800mm F13 G
> '88 54 50 50 0C 0C 4B 06' | = Sigma 50mm F1.4 DG HSM | A
> '89 3C 53 80 30 3C 8B 06' | = AF-S DX Zoom-Nikkor 55-200mm f/4-5.6G ED
> '8A 3C 37 6A 30 30 4B 0E' | = Sigma 24-105mm F4 DG OS HSM
> '8A 54 6A 6A 24 24 8C 0E' | = AF-S VR Micro-Nikkor 105mm f/2.8G IF-ED
> '8B 40 2D 80 2C 3C 8D 0E' | = AF-S DX VR Zoom-Nikkor 18-200mm f/3.5-5.6G IF-ED
> '8B 40 2D 80 2C 3C FD 0E' | = AF-S DX VR Zoom-Nikkor 18-200mm f/3.5-5.6G IF-ED [II]
> '8B 4C 2D 44 14 14 4B 06' | = Sigma 18-35mm F1.8 DC HSM
> '8C 40 2D 53 2C 3C 8E 06' | = AF-S DX Zoom-Nikkor 18-55mm f/3.5-5.6G ED
> '8D 44 5C 8E 34 3C 8F 0E' | = AF-S VR Zoom-Nikkor 70-300mm f/4.5-5.6G IF-ED
> '8E 3C 2B 5C 24 30 4B 0E' | = Sigma 17-70mm F2.8-4 DC Macro OS HSM | C
> '8F 40 2D 72 2C 3C 91 06' | = AF-S DX Zoom-Nikkor 18-135mm f/3.5-5.6G IF-ED
> '8F 48 2B 50 24 24 4B 0E' | = Sigma 17-50mm F2.8 EX DC OS HSM
> '90 3B 53 80 30 3C 92 0E' | = AF-S DX VR Zoom-Nikkor 55-200mm f/4-5.6G IF-ED
> '90 40 2D 80 2C 40 4B 0E' | = Sigma 18-200mm F3.5-6.3 II DC OS HSM
> '91 54 44 44 0C 0C 4B 06' | = Sigma 35mm F1.4 DG HSM
> '92 2C 2D 88 2C 40 4B 0E' | = Sigma 18-250mm F3.5-6.3 DC Macro OS HSM
> '92 48 24 37 24 24 94 06' | = AF-S Zoom-Nikkor 14-24mm f/2.8G ED
> '93 48 37 5C 24 24 95 06' | = AF-S Zoom-Nikkor 24-70mm f/2.8G ED
> '94 40 2D 53 2C 3C 96 06' | = AF-S DX Zoom-Nikkor 18-55mm f/3.5-5.6G ED II
> '94 48 7C 7C 24 24 4B 0E' | = Sigma 180mm F2.8 APO Macro EX DG OS
> '95 00 37 37 2C 2C 97 06' | = PC-E Nikkor 24mm f/3.5D ED
> '95 4C 37 37 2C 2C 97 02' | = PC-E Nikkor 24mm f/3.5D ED
> '96 38 1F 37 34 3C 4B 06' | = Sigma 12-24mm F4.5-5.6 II DG HSM
> '96 48 98 98 24 24 98 0E' | = AF-S VR Nikkor 400mm f/2.8G ED
> '97 3C A0 A0 30 30 99 0E' | = AF-S VR Nikkor 500mm f/4G ED
> '97 48 6A 6A 24 24 4B 0E' | = Sigma Macro 105mm F2.8 EX DG OS HSM
> '98 3C A6 A6 30 30 9A 0E' | = AF-S VR Nikkor 600mm f/4G ED
> '98 48 50 76 24 24 4B 0E' | = Sigma 50-150mm F2.8 EX APO DC OS HSM
> '99 40 29 62 2C 3C 9B 0E' | = AF-S DX VR Zoom-Nikkor 16-85mm f/3.5-5.6G ED
> '99 48 76 76 24 24 4B 0E' | = Sigma APO Macro 150mm F2.8 EX DG OS HSM
> '9A 40 2D 53 2C 3C 9C 0E' | = AF-S DX VR Zoom-Nikkor 18-55mm f/3.5-5.6G
> '9B 00 4C 4C 24 24 9D 06' | = PC-E Micro Nikkor 45mm f/2.8D ED
> '9B 54 4C 4C 24 24 9D 02' | = PC-E Micro Nikkor 45mm f/2.8D ED
> '9B 54 62 62 0C 0C 4B 06' | = Sigma 85mm F1.4 EX DG HSM
> '9C 48 5C 80 24 24 4B 0E' | = Sigma 70-200mm F2.8 EX DG OS HSM
> '9C 54 56 56 24 24 9E 06' | = AF-S Micro Nikkor 60mm f/2.8G ED
> '9D 00 62 62 24 24 9F 06' | = PC-E Micro Nikkor 85mm f/2.8D
> '9D 48 2B 50 24 24 4B 0E' | = Sigma 17-50mm F2.8 EX DC OS HSM
> '9D 54 62 62 24 24 9F 02' | = PC-E Micro Nikkor 85mm f/2.8D
> '9E 38 11 29 34 3C 4B 06' | = Sigma 8-16mm F4.5-5.6 DC HSM
> '9E 40 2D 6A 2C 3C A0 0E' | = AF-S DX VR Zoom-Nikkor 18-105mm f/3.5-5.6G ED
> '9F 37 50 A0 34 40 4B 0E' | = Sigma 50-500mm F4.5-6.3 DG OS HSM
> '9F 58 44 44 14 14 A1 06' | = AF-S DX Nikkor 35mm f/1.8G
> 'A0 40 2D 53 2C 3C CA 0E' | = AF-P DX Nikkor 18-55mm f/3.5-5.6G VR
> 'A0 40 2D 53 2C 3C CA 8E' | = AF-P DX Nikkor 18-55mm f/3.5-5.6G
> 'A0 40 2D 74 2C 3C BB 0E' | = AF-S DX Nikkor 18-140mm f/3.5-5.6G ED VR
> 'A0 48 2A 5C 24 30 4B 0E' | = Sigma 17-70mm F2.8-4 DC Macro OS HSM
> 'A0 54 50 50 0C 0C A2 06' | = AF-S Nikkor 50mm f/1.4G
> 'A1 40 18 37 2C 34 A3 06' | = AF-S DX Nikkor 10-24mm f/3.5-4.5G ED
> 'A1 41 19 31 2C 2C 4B 06' | = Sigma 10-20mm F3.5 EX DC HSM
> 'A1 54 55 55 0C 0C BC 06' | = AF-S Nikkor 58mm f/1.4G
> 'A2 40 2D 53 2C 3C BD 0E' | = AF-S DX Nikkor 18-55mm f/3.5-5.6G VR II
> 'A2 48 5C 80 24 24 A4 0E' | = AF-S Nikkor 70-200mm f/2.8G ED VR II
> 'A3 3C 29 44 30 30 A5 0E' | = AF-S Nikkor 16-35mm f/4G ED VR
> 'A3 3C 5C 8E 30 3C 4B 0E' | = Sigma 70-300mm F4-5.6 DG OS
> 'A4 40 2D 8E 2C 40 BF 0E' | = AF-S DX Nikkor 18-300mm f/3.5-6.3G ED VR
> 'A4 47 2D 50 24 34 4B 0E' | = Sigma 18-50mm F2.8-4.5 DC OS HSM
> 'A4 48 5C 80 24 24 CF 0E' | = AF-S Nikkor 70-200mm f/2.8E FL ED VR
> 'A4 54 37 37 0C 0C A6 06' | = AF-S Nikkor 24mm f/1.4G ED
> 'A5 40 2D 88 2C 40 4B 0E' | = Sigma 18-250mm F3.5-6.3 DC OS HSM
> 'A5 40 3C 8E 2C 3C A7 0E' | = AF-S Nikkor 28-300mm f/3.5-5.6G ED VR
> 'A5 4C 44 44 14 14 C0 06' | = AF-S Nikkor 35mm f/1.8G ED
> 'A5 54 6A 6A 0C 0C D0 06' | = AF-S Nikkor 105mm f/1.4E ED
> 'A5 54 6A 6A 0C 0C D0 46' | = AF-S Nikkor 105mm f/1.4E ED
> 'A6 48 37 5C 24 24 4B 06' | = Sigma 24-70mm F2.8 IF EX DG HSM
> 'A6 48 8E 8E 24 24 A8 0E' | = AF-S VR Nikkor 300mm f/2.8G IF-ED II
> 'A6 48 98 98 24 24 C1 0E' | = AF-S Nikkor 400mm f/2.8E FL ED VR
> 'A7 3C 53 80 30 3C C2 0E' | = AF-S DX Nikkor 55-200mm f/4-5.6G ED VR II
> 'A7 49 80 A0 24 24 4B 06' | = Sigma APO 200-500mm F2.8 EX DG
> 'A7 4B 62 62 2C 2C A9 0E' | = AF-S DX Micro Nikkor 85mm f/3.5G ED VR
> 'A8 38 18 30 34 3C D3 8E' | = AF-P DX Nikkor 10-20mm f/4.5-5.6G VR
> 'A8 48 80 98 30 30 AA 0E' | = AF-S VR Zoom-Nikkor 200-400mm f/4G IF-ED II
> 'A8 48 8E 8E 30 30 C3 0E' | = AF-S Nikkor 300mm f/4E PF ED VR
> 'A8 48 8E 8E 30 30 C3 4E' | = AF-S Nikkor 300mm f/4E PF ED VR
> 'A9 4C 31 31 14 14 C4 06' | = AF-S Nikkor 20mm f/1.8G ED
> 'A9 54 80 80 18 18 AB 0E' | = AF-S Nikkor 200mm f/2G ED VR II
> 'AA 3C 37 6E 30 30 AC 0E' | = AF-S Nikkor 24-120mm f/4G ED VR
> 'AA 48 37 5C 24 24 C5 4E' | = AF-S Nikkor 24-70mm f/2.8E ED VR
> 'AB 3C A0 A0 30 30 C6 4E' | = AF-S Nikkor 500mm f/4E FL ED VR
> 'AC 38 53 8E 34 3C AE 0E' | = AF-S DX VR Nikkor 55-300mm f/4.5-5.6G ED
> 'AC 3C A6 A6 30 30 C7 4E' | = AF-S Nikkor 600mm f/4E FL ED VR
> 'AD 3C 2D 8E 2C 3C AF 0E' | = AF-S DX Nikkor 18-300mm f/3.5-5.6G ED VR
> 'AD 48 28 60 24 30 C8 0E' | = AF-S DX Nikkor 16-80mm f/2.8-4E ED VR
> 'AD 48 28 60 24 30 C8 4E' | = AF-S DX Nikkor 16-80mm f/2.8-4E ED VR
> 'AE 3C 80 A0 3C 3C C9 0E' | = AF-S Nikkor 200-500mm f/5.6E ED VR
> 'AE 3C 80 A0 3C 3C C9 4E' | = AF-S Nikkor 200-500mm f/5.6E ED VR
> 'AE 54 62 62 0C 0C B0 06' | = AF-S Nikkor 85mm f/1.4G
> 'AF 4C 37 37 14 14 CC 06' | = AF-S Nikkor 24mm f/1.8G ED
> 'AF 54 44 44 0C 0C B1 06' | = AF-S Nikkor 35mm f/1.4G
> 'B0 4C 50 50 14 14 B2 06' | = AF-S Nikkor 50mm f/1.8G
> 'B1 48 48 48 24 24 B3 06' | = AF-S DX Micro Nikkor 40mm f/2.8G
> 'B2 48 5C 80 30 30 B4 0E' | = AF-S Nikkor 70-200mm f/4G ED VR
> 'B3 4C 62 62 14 14 B5 06' | = AF-S Nikkor 85mm f/1.8G
> 'B4 40 37 62 2C 34 B6 0E' | = AF-S VR Zoom-Nikkor 24-85mm f/3.5-4.5G IF-ED
> 'B5 4C 3C 3C 14 14 B7 06' | = AF-S Nikkor 28mm f/1.8G
> 'B6 3C B0 B0 3C 3C B8 0E' | = AF-S VR Nikkor 800mm f/5.6E FL ED
> 'B6 3C B0 B0 3C 3C B8 4E' | = AF-S VR Nikkor 800mm f/5.6E FL ED
> 'B6 48 37 56 24 24 1C 02' | = Sigma 24-60mm F2.8 EX DG
> 'B7 44 60 98 34 3C B9 0E' | = AF-S Nikkor 80-400mm f/4.5-5.6G ED VR
> 'B8 40 2D 44 2C 34 BA 06' | = AF-S Nikkor 18-35mm f/3.5-4.5G ED
> 'BF 4E 26 26 1E 1E 01 04' | = Irix 15mm f/2.4 Firefly
> 'C3 34 68 98 38 40 4B 4E' | = Sigma 100-400mm F5-6.3 DG OS HSM | C
> 'CC 4C 50 68 14 14 4B 06' | = Sigma 50-100mm F1.8 DC HSM | A
> 'CD 3D 2D 70 2E 3C 4B 0E' | = Sigma 18-125mm F3.8-5.6 DC OS HSM
> 'CE 34 76 A0 38 40 4B 0E' | = Sigma 150-500mm F5-6.3 DG OS APO HSM
> 'CF 38 6E 98 34 3C 4B 0E' | = Sigma APO 120-400mm F4.5-5.6 DG OS HSM
> 'DC 48 19 19 24 24 4B 06' | = Sigma 10mm F2.8 EX DC HSM Fisheye
> 'DE 54 50 50 0C 0C 4B 06' | = Sigma 50mm F1.4 EX DG HSM
> 'E0 3C 5C 8E 30 3C 4B 06' | = Sigma 70-300mm F4-5.6 APO DG Macro HSM
> 'E1 58 37 37 14 14 1C 02' | = Sigma 24mm F1.8 EX DG Aspherical Macro
> 'E3 40 76 A6 38 40 DF 4E' | = Tamron SP 150-600mm f/5-6.3 Di VC USD G2
> 'E3 54 50 50 24 24 35 02' | = Sigma Macro 50mm F2.8 EX DG
> 'E4 54 64 64 24 24 DF 0E' | = Tamron SP 90mm f/2.8 Di VC USD Macro 1:1 (F017)
> 'E5 54 6A 6A 24 24 35 02' | = Sigma Macro 105mm F2.8 EX DG
> 'E6 40 2D 80 2C 40 DF 0E' | = Tamron AF 18-200mm f/3.5-6.3 Di II VC (B018)
> 'E6 41 3C 8E 2C 40 1C 02' | = Sigma 28-300mm F3.5-6.3 DG Macro
> 'E7 4C 4C 4C 14 14 DF 0E' | = Tamron SP 45mm f/1.8 Di VC USD (F013)
> 'E8 4C 44 44 14 14 DF 0E' | = Tamron SP 35mm f/1.8 Di VC USD (F012)
> 'E9 48 27 3E 24 24 DF 0E' | = Tamron SP 15-30mm f/2.8 Di VC USD (A012)
> 'E9 54 37 5C 24 24 1C 02' | = Sigma 24-70mm F2.8 EX DG Macro
> 'EA 40 29 8E 2C 40 DF 0E' | = Tamron AF 16-300mm f/3.5-6.3 Di II VC PZD (B016)
> 'EA 48 27 27 24 24 1C 02' | = Sigma 15mm F2.8 EX Diagonal Fisheye
> 'EB 40 76 A6 38 40 DF 0E' | = Tamron SP AF 150-600mm f/5-6.3 VC USD (A011)
> 'ED 40 2D 80 2C 40 4B 0E' | = Sigma 18-200mm F3.5-6.3 DC OS HSM
> 'EE 48 5C 80 24 24 4B 06' | = Sigma 70-200mm F2.8 EX APO DG Macro HSM II
> 'F0 38 1F 37 34 3C 4B 06' | = Sigma 12-24mm F4.5-5.6 EX DG Aspherical HSM
> 'F0 3F 2D 8A 2C 40 DF 0E' | = Tamron AF 18-270mm f/3.5-6.3 Di II VC PZD (B008)
> 'F1 44 A0 A0 34 34 4B 02' | = Sigma APO 500mm F4.5 EX DG HSM
> 'F1 47 5C 8E 30 3C DF 0E' | = Tamron SP 70-300mm f/4-5.6 Di VC USD (A005)
> 'F3 48 68 8E 30 30 4B 02' | = Sigma APO 100-300mm F4 EX IF HSM
> 'F3 54 2B 50 24 24 84 0E' | = Tamron SP AF 17-50mm f/2.8 XR Di II VC LD Aspherical (IF) (B005)
> 'F4 54 56 56 18 18 84 06' | = Tamron SP AF 60mm f/2.0 Di II Macro 1:1 (G005)
> 'F5 40 2C 8A 2C 40 40 0E' | = Tamron AF 18-270mm f/3.5-6.3 Di II VC LD Aspherical (IF) Macro (B003)
> 'F5 48 76 76 24 24 4B 06' | = Sigma APO Macro 150mm F2.8 EX DG HSM
> 'F6 3F 18 37 2C 34 84 06' | = Tamron SP AF 10-24mm f/3.5-4.5 Di II LD Aspherical (IF) (B001)
> 'F6 3F 18 37 2C 34 DF 06' | = Tamron SP AF 10-24mm f/3.5-4.5 Di II LD Aspherical (IF) (B001)
> 'F6 48 2D 50 24 24 4B 06' | = Sigma 18-50mm F2.8 EX DC Macro
> 'F7 53 5C 80 24 24 40 06' | = Tamron SP AF 70-200mm f/2.8 Di LD (IF) Macro (A001)
> 'F7 53 5C 80 24 24 84 06' | = Tamron SP AF 70-200mm f/2.8 Di LD (IF) Macro (A001)
> 'F8 54 3E 3E 0C 0C 4B 06' | = Sigma 30mm F1.4 EX DC HSM
> 'F8 54 64 64 24 24 DF 06' | = Tamron SP AF 90mm f/2.8 Di Macro 1:1 (272NII)
> 'F8 55 64 64 24 24 84 06' | = Tamron SP AF 90mm f/2.8 Di Macro 1:1 (272NII)
> 'F9 3C 19 31 30 3C 4B 06' | = Sigma 10-20mm F4-5.6 EX DC HSM
> 'F9 40 3C 8E 2C 40 40 0E' | = Tamron AF 28-300mm f/3.5-6.3 XR Di VC LD Aspherical (IF) Macro (A20)
> 'FA 54 3C 5E 24 24 84 06' | = Tamron SP AF 28-75mm f/2.8 XR Di LD Aspherical (IF) Macro (A09NII)
> 'FA 54 3C 5E 24 24 DF 06' | = Tamron SP AF 28-75mm f/2.8 XR Di LD Aspherical (IF) Macro (A09NII)
> 'FA 54 6E 8E 24 24 4B 02' | = Sigma APO 120-300mm F2.8 EX DG HSM
> 'FB 54 2B 50 24 24 84 06' | = Tamron SP AF 17-50mm f/2.8 XR Di II LD Aspherical (IF) (A16NII)
> 'FB 54 8E 8E 24 24 4B 02' | = Sigma APO 300mm F2.8 EX DG HSM
> 'FC 40 2D 80 2C 40 DF 06' | = Tamron AF 18-200mm f/3.5-6.3 XR Di II LD Aspherical (IF) Macro (A14NII)
> 'FD 47 50 76 24 24 4B 06' | = Sigma 50-150mm F2.8 EX APO DC HSM II
> 'FE 47 00 00 24 24 4B 06' | = Sigma 4.5mm F2.8 EX DC HSM Circular Fisheye
> 'FE 48 37 5C 24 24 DF 0E' | = Tamron SP 24-70mm f/2.8 Di VC USD (A007)
> 'FE 53 5C 80 24 24 84 06' | = Tamron SP AF 70-200mm f/2.8 Di LD (IF) Macro (A001)
> 'FE 54 5C 80 24 24 DF 0E' | = Tamron SP 70-200mm f/2.8 Di VC USD (A009)
> 'FE 54 64 64 24 24 DF 0E' | = Tamron SP 90mm f/2.8 Di VC USD Macro 1:1 (F004)
> 'FF 40 2D 80 2C 40 4B 06' | = Sigma 18-200mm F3.5-6.3 DC

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Oct 26, 2017

<-- ExifTool Tag Names